<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<library>
<packages>
<package name="68610614122">
<description>&lt;b&gt;WR-FPC 1.00mm SMT ZIF Horizontal Top Contact, 6 Pins
&lt;p&gt;&lt;b&gt;Digikey Part #: &lt;a href="https://www.digikey.ca/product-detail/en/molex-llc/0522070660/WM10939CT-ND/5170941" targe="blank"&gt;WM10939CT-ND&lt;a/&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;Added: 2019 03 15. C. D'Arcy&lt;/p&gt;</description>
</package>
<package name="TACTILE_BUTTON_SMD_5.2MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 5.2mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/Buttons/SMD-Button.pdf"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="SOIC_16_N">
<description>SOIC, 3.9mm (0.15in) width</description>
</package>
<package name="4816P">
<description>&lt;b&gt;BOURNS RESISTOR NETWORK&lt;/b&gt;</description>
</package>
<package name="SO14">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="LED_1206">
</package>
<package name="ISP_PADS">
</package>
<package name="PAD_GND">
<description>&lt;b&gt;SMD GND PAD&lt;/b&gt;</description>
</package>
<package name="PAD_VCC">
<description>&lt;b&gt;SMD VCC PAD&lt;/b&gt;</description>
</package>
<package name="SOT223">
<description>&lt;b&gt;Smal Outline Transistor&lt;/b&gt;</description>
</package>
<package name="RESISTOR_1206">
<description>&lt;p&gt;&lt;b&gt;Generic 3216 (1206) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="SOIC_20_W">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
wide body 7.5 mm/JEDEC MS-013AC</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="SO08">
<description>SOIC, 3.8mm (0.15 inch) width</description>
</package>
<package name="SO24W">
<description>&lt;b&gt;Wide Small Outline package&lt;/b&gt; 300 mil</description>
</package>
<package name="SO16">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
<package name="SOIC127P1032X265-20">
<description>20-SOIC, 1.27 mm pitch, 10.32 mm span, 12.80 X 7.50 X 2.65 mm body
&lt;p&gt;20-pin SOIC package with 1.27 mm pitch, 10.32 mm span with body size 12.80 X 7.50 X 2.65 mm&lt;/p&gt;</description>
</package>
<package name="SOIC127P798X216-8">
<description>8-SOIC, 1.27 mm pitch, 7.98 mm span, 4.89 X 5.29 X 2.16 mm body
&lt;p&gt;8-pin SOIC package with 1.27 mm pitch, 7.98 mm span with body size 4.89 X 5.29 X 2.16 mm&lt;/p&gt;</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="SO28W">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
wide body 7.5 mm/JEDEC MO-119AB</description>
</package>
<package name="SO20W">
<description>&lt;b&gt;Wide Small Outline package&lt;/b&gt; 300 mil</description>
</package>
<package name="EG1390">
</package>
<package name="0603-RED">
</package>
<package name="SOIC8">
<description>&lt;b&gt;Small Outline IC&lt;/b&gt;</description>
</package>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="5501">
<description>&lt;b&gt;PUSHBUTTON SERIES 5500 SWITCHES&lt;/b&gt;&lt;p&gt;
Source: www.e-switch.com .. 5500.pdf</description>
</package>
<package name="693063010911">
<description>&lt;B&gt;WR-CRD&lt;/B&gt;&lt;BR&gt;
SD CARD CONNECTOR&lt;BR&gt;
PUSH &amp; PULL&lt;BR&gt;
WITH CARD DETECTION&lt;BR&gt;
9PINS</description>
</package>
<package name="USB-AB-MICRO-SMD">
<description>&lt;h3&gt;USB Type AB - SMT&lt;/h3&gt;
&lt;br&gt; Basic silk outline&lt;/br&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5 main, 3 shield&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint: http://www.morethanall.com//upload/products_pdf/87340574052ba5151280ca.pdf&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB AB&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="UX60-MB-5ST">
<description>&lt;b&gt;MINI USB Connector HI-SPEED Certified&lt;/b&gt; Metal Shield SMT Type With Positioning Post&lt;p&gt;
Source: http://www.hirose.co.jp/cataloge_hp/e24000019.pdf</description>
</package>
<package name="SMALL_TSILK_TEXT">
</package>
<package name="TINY_BSILK_TEXT">
</package>
<package name="MOUNTINGHOLE_3.2MM_PLATEDTHIN">
</package>
<package name="MEDIUM_TSILK_TEXT">
</package>
<package name="MEDIUM_TSILK">
</package>
<package name="SMALL_TSILK">
</package>
<package name="TINY_TSILK">
</package>
<package name="MEDIUM_BSILK">
</package>
<package name="MEDIUM_BSILK_TEXT">
</package>
<package name="SMALL_BSILK">
</package>
<package name="SMALL_BSILK_TEXT">
</package>
<package name="TINY_BSILK">
</package>
<package name="TINY_TSILK_TEXT">
</package>
</packages>
<symbols>
<symbol name="6-ISP">
<pin name="MISO" direction="pas"/>
<pin name="5V+" direction="pas"/>
<pin name="SCK" direction="pas"/>
<pin name="MOSI" direction="pas"/>
<pin name="RESET" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="SWITCH-MOMENTARY">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - Two Circuits&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons). Schematic symbol includes two switch circuits.&lt;/p&gt;</description>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="TPIC6C595">
<pin name="!CLR" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="RCK" direction="in"/>
<pin name="SER_IN" direction="in"/>
<pin name="SER_OUT" direction="out"/>
<pin name="SRCK" direction="in"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="74595">
<pin name="QB" direction="hiz"/>
<pin name="QC" direction="hiz"/>
<pin name="QD" direction="hiz"/>
<pin name="QE" direction="hiz"/>
<pin name="QF" direction="hiz"/>
<pin name="QG" direction="hiz"/>
<pin name="QH" direction="hiz"/>
<pin name="SCL" direction="in" function="dot"/>
<pin name="SCK" direction="in" function="clk"/>
<pin name="RCK" direction="in" function="clk"/>
<pin name="G" direction="in" function="dot"/>
<pin name="SER" direction="in"/>
<pin name="QA" direction="hiz"/>
<pin name="QH*" direction="hiz"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="RX10">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
</symbol>
<symbol name="RX08">
<pin name="1" direction="in"/>
<pin name="2" direction="in"/>
<pin name="3" direction="in"/>
<pin name="4" direction="in"/>
<pin name="5" direction="in"/>
<pin name="6" direction="in"/>
<pin name="7" direction="in"/>
<pin name="8" direction="in"/>
<pin name="9" direction="out"/>
<pin name="10" direction="out"/>
<pin name="11" direction="out"/>
<pin name="12" direction="out"/>
<pin name="13" direction="out"/>
<pin name="14" direction="out"/>
<pin name="15" direction="out"/>
<pin name="16" direction="out"/>
</symbol>
<symbol name="ATTINY84">
<pin name="VCC"/>
<pin name="(PCINT3/T0/ADC3)PA3"/>
<pin name="(PCINT2/AIN1/ADC2)PA2"/>
<pin name="(PCINT1/AIN0/ADC1)PA1"/>
<pin name="(PCINT0/AREF/ADC0)PA0"/>
<pin name="(PCINT4/T1/SCL/USCK/ADC4)PA4"/>
<pin name="(PCINT5/OC1B/MISO/DO/ADC5)PA5"/>
<pin name="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6"/>
<pin name="(PCINT7/ICP/OC0B/ADC7)PA7"/>
<pin name="(PCINT8/XTAL1/CLKI)PB0"/>
<pin name="(PCINT9/XTAL2)PB1"/>
<pin name="(PCINT10/INT0/OC0A/CKOUT)PB2"/>
<pin name="(PCINT11/~RESET/DW)PB3"/>
<pin name="GND"/>
</symbol>
<symbol name="ATMEGAXX8-32PIN_NOPAD">
<pin name="PB5(SCK)"/>
<pin name="PB7(XTAL2/TOSC2)"/>
<pin name="PB6(XTAL1/TOSC1)"/>
<pin name="GND@3"/>
<pin name="GND@5"/>
<pin name="VCC@4"/>
<pin name="VCC@6"/>
<pin name="AGND"/>
<pin name="AREF"/>
<pin name="AVCC"/>
<pin name="PB4(MISO)"/>
<pin name="PB3(MOSI/OC2)"/>
<pin name="PB2(SS/OC1B)"/>
<pin name="PB1(OC1A)"/>
<pin name="PB0(ICP)"/>
<pin name="PD7(AIN1)"/>
<pin name="PD6(AIN0)"/>
<pin name="PD5(T1)"/>
<pin name="PD4(XCK/T0)"/>
<pin name="PD3(INT1)"/>
<pin name="PD2(INT0)"/>
<pin name="PD1(TXD)"/>
<pin name="PD0(RXD)"/>
<pin name="ADC7"/>
<pin name="ADC6"/>
<pin name="PC5(ADC5/SCL)"/>
<pin name="PC4(ADC4/SDA)"/>
<pin name="PC3(ADC3)"/>
<pin name="PC2(ADC2)"/>
<pin name="PC1(ADC1)"/>
<pin name="PC0(ADC0)"/>
<pin name="PC6(/RESET)" function="dot"/>
</symbol>
<symbol name="TINY13">
<pin name="PB5/PCINT5/!RESET!/ADC0/DW"/>
<pin name="PB3/PCINT3/CLKI/ADC3"/>
<pin name="PB4/PCINT4/ADC2"/>
<pin name="PB0/PCINT0/AIN0/OC0A/MOSI"/>
<pin name="PB1/PCINT1/AIN1/OC0B/INT0/MISO"/>
<pin name="PB2/PCINT2/SCK/ADC1/T0"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="LED">
<description>&lt;h3&gt;LED&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;</description>
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="PAD">
<pin name="P" direction="pas"/>
</symbol>
<symbol name="REG1117">
<pin name="VIN" direction="in"/>
<pin name="VOUT" direction="out"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="RESISTOR">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="L293DD">
<pin name="EN1" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="OUT2" direction="out"/>
<pin name="IN2" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="IN3" direction="in"/>
<pin name="OUT4" direction="out"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="OUT3" direction="out"/>
<pin name="IN4" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
</symbol>
<symbol name="SOIC20">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="P$15"/>
<pin name="P$16"/>
<pin name="P$17"/>
<pin name="P$18"/>
<pin name="P$19"/>
<pin name="P$20"/>
</symbol>
<symbol name="SOIC16">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="P$15"/>
<pin name="P$16"/>
</symbol>
<symbol name="SOIC14">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
</symbol>
<symbol name="SOIC8">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
</symbol>
<symbol name="C_US_NONPOLAR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="C_US_POLAR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="NE555">
<pin name="TRE" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="DIS" direction="in"/>
<pin name="TRI" direction="in"/>
<pin name="VCC+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="CON" direction="in"/>
<pin name="/RES" direction="in"/>
</symbol>
<symbol name="SOIC24">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="P$15"/>
<pin name="P$16"/>
<pin name="P$17"/>
<pin name="P$18"/>
<pin name="P$19"/>
<pin name="P$20"/>
<pin name="P$21"/>
<pin name="P$22"/>
<pin name="P$23"/>
<pin name="P$24"/>
</symbol>
<symbol name="MICRO_USB_AB">
<description>&lt;h3&gt;USB Type AB&lt;/h3&gt;
&lt;p&gt;Capable of OTG. 
&lt;br&gt;5-pins: USBVCC, GND, D+, D-, USBID&lt;/p&gt;</description>
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="USBID"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="MINI_USB">
<pin name="5V" direction="in"/>
<pin name="2" direction="in"/>
<pin name="3" direction="in"/>
<pin name="4" direction="in"/>
<pin name="GND" direction="in"/>
</symbol>
<symbol name="LOGO">
</symbol>
<symbol name="MOUNTING_HOLE">
</symbol>
</symbols>
<devicesets>
<deviceset name="CONN_FPC_ISP" prefix="J" uservalue="yes">
<description>&lt;b&gt;WR-FPC 1.00mm SMT ZIF Horizontal Top Contact, 6 Pins&lt;/b&gt;=&gt;Code : Con_FPC_ZIF_1.00_68610614122
&lt;br&gt;&lt;a href="http://katalog.we-online.de/media/images/eican/Con_FPC_ZIF_1.00_6861xx14122_pf2.jpg" title="Enlarge picture"&gt;
&lt;img src="http://katalog.we-online.de/media/thumbs2/eican/thb_Con_FPC_ZIF_1.00_6861xx14122_pf2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/em/686_1xx_141_22"&gt;http://katalog.we-online.de/en/em/686_1xx_141_22&lt;/a&gt;&lt;p&gt;
Created 2014-07-09, Karrer Zheng&lt;br&gt;
2014 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="6-ISP"/>
</gates>
<devices>
<device name="CONNECTOR_PADS" package="68610614122">
<connects>
<connect gate="G$1" pin="5V+" pad="5V+"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="RESET" pad="RESET"/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PADS_ONLY" package="ISP_PADS">
<connects>
<connect gate="G$1" pin="5V+" pad="5V+"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="RESET" pad="RESET"/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TACTILE_BUTTON">
<gates>
<gate name="G$1" symbol="SWITCH-MOMENTARY"/>
</gates>
<devices>
<device name="" package="TACTILE_BUTTON_SMD_5.2MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="595">
<description>&lt;b&gt;Texas Instruments Part #:&lt;/b&gt; &lt;a href="http://www.ti.com/lit/ds/symlink/sn74ahc595.pdf"&gt;SN74AHC595D&lt;/a&gt;&lt;br&gt;

&lt;b&gt;Digikey Part#:&lt;/b&gt; &lt;a href="https://www.digikey.ca/product-detail/en/SN74AHC595D/296-4618-5-ND/375884/?itemSeq=256350752"&gt;296-4618-5-ND&lt;/a&gt;&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="74595"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$1" pin="G" pad="13"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="QA" pad="15"/>
<connect gate="G$1" pin="QB" pad="1"/>
<connect gate="G$1" pin="QC" pad="2"/>
<connect gate="G$1" pin="QD" pad="3"/>
<connect gate="G$1" pin="QE" pad="4"/>
<connect gate="G$1" pin="QF" pad="5"/>
<connect gate="G$1" pin="QG" pad="6"/>
<connect gate="G$1" pin="QH" pad="7"/>
<connect gate="G$1" pin="QH*" pad="9"/>
<connect gate="G$1" pin="RCK" pad="12"/>
<connect gate="G$1" pin="SCK" pad="11"/>
<connect gate="G$1" pin="SCL" pad="10"/>
<connect gate="G$1" pin="SER" pad="14"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESISTOR_NETWORK" prefix="R">
<description>&lt;b&gt;BOURNS RESISTOR NETWORK&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="RX08"/>
</gates>
<devices>
<device name="" package="4816P">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="BOURNS, INC."/>
<attribute name="MPN" value="4816P-T01-684LF"/>
<attribute name="OC_FARNELL" value="9357483"/>
<attribute name="OC_NEWARK" value="33K0707"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY84_SO14">
<gates>
<gate name="G$1" symbol="ATTINY84"/>
</gates>
<devices>
<device name="" package="SO14">
<connects>
<connect gate="G$1" pin="(PCINT0/AREF/ADC0)PA0" pad="13"/>
<connect gate="G$1" pin="(PCINT1/AIN0/ADC1)PA1" pad="12"/>
<connect gate="G$1" pin="(PCINT10/INT0/OC0A/CKOUT)PB2" pad="5"/>
<connect gate="G$1" pin="(PCINT11/~RESET/DW)PB3" pad="4"/>
<connect gate="G$1" pin="(PCINT2/AIN1/ADC2)PA2" pad="11"/>
<connect gate="G$1" pin="(PCINT3/T0/ADC3)PA3" pad="10"/>
<connect gate="G$1" pin="(PCINT4/T1/SCL/USCK/ADC4)PA4" pad="9"/>
<connect gate="G$1" pin="(PCINT5/OC1B/MISO/DO/ADC5)PA5" pad="8"/>
<connect gate="G$1" pin="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6" pad="7"/>
<connect gate="G$1" pin="(PCINT7/ICP/OC0B/ADC7)PA7" pad="6"/>
<connect gate="G$1" pin="(PCINT8/XTAL1/CLKI)PB0" pad="2"/>
<connect gate="G$1" pin="(PCINT9/XTAL2)PB1" pad="3"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA328P_TQFP32" prefix="U">
<description>&lt;h3&gt;Popular 328P in QFP&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/13448"&gt;Storefront component: ATmega328 - TQFP&lt;/a&gt; (COM-13448)&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.sparkfun.com/datasheets/Components/SMD/ATMega328.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12757"&gt;SparkFun RedBoard - Programmed with Arduino&lt;/a&gt; (DEV-12757)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11113"&gt;Arduino Pro Mini 328 - 5V/16MHz&lt;/a&gt; (DEV-11113)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11114"&gt;Arduino Pro Mini 328 - 3.3V/8MHz&lt;/a&gt; (DEV-11114)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13712"&gt;SparkFun OpenLog&lt;/a&gt; (DEV-13712)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12923"&gt;SparkFun MicroView - OLED Arduino Module&lt;/a&gt; (DEV-12923)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12651"&gt;SparkFun Digital Sandbox&lt;/a&gt; (DEV-12651)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11888"&gt;SparkFun PicoBoard&lt;/a&gt; (WIG-11888)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10116"&gt;Arduino Fio&lt;/a&gt; (DEV-10116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13342"&gt;LilyPad Arduino 328 Main Board&lt;/a&gt; (DEV-13342)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13741"&gt;SparkFun RedStick&lt;/a&gt; (DEV-13741)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11013"&gt;LilyPad MP3&lt;/a&gt; (DEV-11013)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10941"&gt;LilyPad Arduino SimpleSnap&lt;/a&gt; (DEV-10941)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13899"&gt;SparkFun Stepoko&lt;/a&gt; (ROB-13899)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11345"&gt;SparkFun Geiger Counter&lt;/a&gt; (SEN-11345)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12781"&gt;SparkFun EL Sequencer&lt;/a&gt; (COM-12781)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10915"&gt;Arduino Pro 328 - 5V/16MHz&lt;/a&gt; (DEV-10915)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12773"&gt;CryptoCape&lt;/a&gt; (DEV-12773)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10740"&gt;SparkFun IR Thermometer Evaluation Board - MLX90614&lt;/a&gt; (SEN-10740)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12097"&gt;SparkFun RedBot Mainboard&lt;/a&gt; (ROB-12097)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10914"&gt;Arduino Pro 328 - 3.3V/8MHz&lt;/a&gt; (DEV-10914)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13036"&gt;SparkFun Block for Intel® Edison - Arduino&lt;/a&gt; (DEV-13036)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10935"&gt;SparkFun Simon Says - Surface Mount Soldering Kit&lt;/a&gt; (KIT-10935)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11441"&gt;SparkFun 7-Segment Serial Display - Red&lt;/a&gt; (COM-11441)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11629"&gt;SparkFun 7-Segment Serial Display - White&lt;/a&gt; (COM-11629)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11443"&gt;SparkFun 7-Segment Serial Display - Yellow&lt;/a&gt; (COM-11443)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11440"&gt;SparkFun 7-Segment Serial Display - Kelly Green&lt;/a&gt; (COM-11440)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11442"&gt;SparkFun 7-Segment Serial Display - Blue&lt;/a&gt; (COM-11442)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11647"&gt;SparkFun OpenSegment Serial Display - 20mm (Blue)&lt;/a&gt; (COM-11647)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11646"&gt;SparkFun OpenSegment Serial Display - 20mm (Green)&lt;/a&gt; (COM-11646)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11648"&gt;SparkFun OpenSegment Serial Display - 20mm (White)&lt;/a&gt; (COM-11648)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11644"&gt;SparkFun OpenSegment Serial Display - 20mm (Red)&lt;/a&gt; (COM-11644)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11645"&gt;SparkFun OpenSegment Serial Display - 20mm (Yellow)&lt;/a&gt; (COM-11645)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13190"&gt;SparkFun OpenSegment Shield&lt;/a&gt; (DEV-13190)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="U$1" symbol="ATMEGAXX8-32PIN_NOPAD"/>
</gates>
<devices>
<device name="" package="TQFP32-08">
<connects>
<connect gate="U$1" pin="ADC6" pad="19"/>
<connect gate="U$1" pin="ADC7" pad="22"/>
<connect gate="U$1" pin="AGND" pad="21"/>
<connect gate="U$1" pin="AREF" pad="20"/>
<connect gate="U$1" pin="AVCC" pad="18"/>
<connect gate="U$1" pin="GND@3" pad="3"/>
<connect gate="U$1" pin="GND@5" pad="5"/>
<connect gate="U$1" pin="PB0(ICP)" pad="12"/>
<connect gate="U$1" pin="PB1(OC1A)" pad="13"/>
<connect gate="U$1" pin="PB2(SS/OC1B)" pad="14"/>
<connect gate="U$1" pin="PB3(MOSI/OC2)" pad="15"/>
<connect gate="U$1" pin="PB4(MISO)" pad="16"/>
<connect gate="U$1" pin="PB5(SCK)" pad="17"/>
<connect gate="U$1" pin="PB6(XTAL1/TOSC1)" pad="7"/>
<connect gate="U$1" pin="PB7(XTAL2/TOSC2)" pad="8"/>
<connect gate="U$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="U$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="U$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="U$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="U$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="U$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="U$1" pin="PC6(/RESET)" pad="29"/>
<connect gate="U$1" pin="PD0(RXD)" pad="30"/>
<connect gate="U$1" pin="PD1(TXD)" pad="31"/>
<connect gate="U$1" pin="PD2(INT0)" pad="32"/>
<connect gate="U$1" pin="PD3(INT1)" pad="1"/>
<connect gate="U$1" pin="PD4(XCK/T0)" pad="2"/>
<connect gate="U$1" pin="PD5(T1)" pad="9"/>
<connect gate="U$1" pin="PD6(AIN0)" pad="10"/>
<connect gate="U$1" pin="PD7(AIN1)" pad="11"/>
<connect gate="U$1" pin="VCC@4" pad="4"/>
<connect gate="U$1" pin="VCC@6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY85_SO8">
<gates>
<gate name="G$1" symbol="TINY13"/>
</gates>
<devices>
<device name="" package="SOIC127P798X216-8">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0/PCINT0/AIN0/OC0A/MOSI" pad="5"/>
<connect gate="G$1" pin="PB1/PCINT1/AIN1/OC0B/INT0/MISO" pad="6"/>
<connect gate="G$1" pin="PB2/PCINT2/SCK/ADC1/T0" pad="7"/>
<connect gate="G$1" pin="PB3/PCINT3/CLKI/ADC3" pad="2"/>
<connect gate="G$1" pin="PB4/PCINT4/ADC2" pad="3"/>
<connect gate="G$1" pin="PB5/PCINT5/!RESET!/ADC0/DW" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED_1206" prefix="LED">
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="LED_1206">
<connects>
<connect gate="G$1" pin="A" pad="+"/>
<connect gate="G$1" pin="C" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PAD_SINGLE">
<gates>
<gate name="G$1" symbol="PAD"/>
</gates>
<devices>
<device name="GND" package="PAD_GND">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VCC" package="PAD_VCC">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="5VREG" prefix="U" uservalue="yes">
<description>&lt;b&gt;800mA Low Dropout (LDO) Positive Regulator&lt;/b&gt;&lt;p&gt;
with Current Source and Sink Capability</description>
<gates>
<gate name="G$1" symbol="REG1117"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VIN" pad="3"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="REG1118-2.85/2K5G4"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="14M2185"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESISTOR">
<gates>
<gate name="G$1" symbol="RESISTOR"/>
</gates>
<devices>
<device name="" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L293DD_MOTOR" prefix="IC">
<description>&lt;b&gt;PUSH-PULL FOUR CHANNEL DRIVER WITH DIODES&lt;/b&gt;&lt;p&gt;
Source: http://www.st.com/stonline/books/pdf/docs/1330.pdf</description>
<gates>
<gate name="G$1" symbol="L293DD"/>
</gates>
<devices>
<device name="" package="SOIC_20_W">
<connects>
<connect gate="G$1" pin="EN1" pad="1"/>
<connect gate="G$1" pin="EN2" pad="11"/>
<connect gate="G$1" pin="GND@1" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="GND@3" pad="6"/>
<connect gate="G$1" pin="GND@4" pad="7"/>
<connect gate="G$1" pin="GND@5" pad="14"/>
<connect gate="G$1" pin="GND@6" pad="15"/>
<connect gate="G$1" pin="GND@7" pad="16"/>
<connect gate="G$1" pin="GND@8" pad="17"/>
<connect gate="G$1" pin="IN1" pad="2"/>
<connect gate="G$1" pin="IN2" pad="9"/>
<connect gate="G$1" pin="IN3" pad="12"/>
<connect gate="G$1" pin="IN4" pad="19"/>
<connect gate="G$1" pin="OUT1" pad="3"/>
<connect gate="G$1" pin="OUT2" pad="8"/>
<connect gate="G$1" pin="OUT3" pad="13"/>
<connect gate="G$1" pin="OUT4" pad="18"/>
<connect gate="G$1" pin="VS" pad="10"/>
<connect gate="G$1" pin="VSS" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOIC20_W" prefix="IC">
<gates>
<gate name="G$1" symbol="SOIC20"/>
</gates>
<devices>
<device name="" package="SO20W">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$10" pad="10"/>
<connect gate="G$1" pin="P$11" pad="11"/>
<connect gate="G$1" pin="P$12" pad="12"/>
<connect gate="G$1" pin="P$13" pad="13"/>
<connect gate="G$1" pin="P$14" pad="14"/>
<connect gate="G$1" pin="P$15" pad="15"/>
<connect gate="G$1" pin="P$16" pad="16"/>
<connect gate="G$1" pin="P$17" pad="17"/>
<connect gate="G$1" pin="P$18" pad="18"/>
<connect gate="G$1" pin="P$19" pad="19"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$20" pad="20"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$5" pad="5"/>
<connect gate="G$1" pin="P$6" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
<connect gate="G$1" pin="P$9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOIC16" prefix="IC">
<gates>
<gate name="G$1" symbol="SOIC16"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$10" pad="10"/>
<connect gate="G$1" pin="P$11" pad="11"/>
<connect gate="G$1" pin="P$12" pad="12"/>
<connect gate="G$1" pin="P$13" pad="13"/>
<connect gate="G$1" pin="P$14" pad="14"/>
<connect gate="G$1" pin="P$15" pad="15"/>
<connect gate="G$1" pin="P$16" pad="16"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$5" pad="5"/>
<connect gate="G$1" pin="P$6" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
<connect gate="G$1" pin="P$9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAPACITOR_1206_NONPPOLAR" prefix="C">
<gates>
<gate name="G$1" symbol="C_US_NONPOLAR"/>
</gates>
<devices>
<device name="" package="C1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAPACITOR_1206_POLAR" prefix="C">
<gates>
<gate name="G$1" symbol="C_US_POLAR"/>
</gates>
<devices>
<device name="" package="C1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="555">
<gates>
<gate name="G$1" symbol="NE555"/>
</gates>
<devices>
<device name="SIMPLE" package="SO08">
<connects>
<connect gate="G$1" pin="/RES" pad="4"/>
<connect gate="G$1" pin="CON" pad="5"/>
<connect gate="G$1" pin="DIS" pad="7"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="TRE" pad="6"/>
<connect gate="G$1" pin="TRI" pad="2"/>
<connect gate="G$1" pin="VCC+" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOIC24_W">
<gates>
<gate name="G$1" symbol="SOIC24"/>
</gates>
<devices>
<device name="" package="SO24W">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$10" pad="10"/>
<connect gate="G$1" pin="P$11" pad="11"/>
<connect gate="G$1" pin="P$12" pad="12"/>
<connect gate="G$1" pin="P$13" pad="13"/>
<connect gate="G$1" pin="P$14" pad="14"/>
<connect gate="G$1" pin="P$15" pad="15"/>
<connect gate="G$1" pin="P$16" pad="16"/>
<connect gate="G$1" pin="P$17" pad="17"/>
<connect gate="G$1" pin="P$18" pad="18"/>
<connect gate="G$1" pin="P$19" pad="19"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$20" pad="20"/>
<connect gate="G$1" pin="P$21" pad="21"/>
<connect gate="G$1" pin="P$22" pad="22"/>
<connect gate="G$1" pin="P$23" pad="23"/>
<connect gate="G$1" pin="P$24" pad="24"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$5" pad="5"/>
<connect gate="G$1" pin="P$6" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
<connect gate="G$1" pin="P$9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPIC6C595">
<gates>
<gate name="G$1" symbol="TPIC6C595"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$1" pin="!CLR" pad="7"/>
<connect gate="G$1" pin="!G" pad="8"/>
<connect gate="G$1" pin="D0" pad="3"/>
<connect gate="G$1" pin="D1" pad="4"/>
<connect gate="G$1" pin="D2" pad="5"/>
<connect gate="G$1" pin="D3" pad="6"/>
<connect gate="G$1" pin="D4" pad="11"/>
<connect gate="G$1" pin="D5" pad="12"/>
<connect gate="G$1" pin="D6" pad="13"/>
<connect gate="G$1" pin="D7" pad="14"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="RCK" pad="10"/>
<connect gate="G$1" pin="SER_IN" pad="2"/>
<connect gate="G$1" pin="SER_OUT" pad="9"/>
<connect gate="G$1" pin="SRCK" pad="15"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MICRO_USB_AB" prefix="J" uservalue="yes">
<description>&lt;h3&gt;USB Type AB Micro Connector&lt;/h3&gt;
&lt;p&gt;OTG-compatible. 5 pins, 3 shield pins&lt;/p&gt;

&lt;p&gt;&lt;b&gt;Digikey Part#:&lt;/b&gt; &lt;a href="https://www.digikey.ca/product-detail/en/hirose-electric-co-ltd/ZX62-AB-5PA-31/H125279CT-ND/5994741"&gt; H125279CT-ND&lt;/a&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MICRO_USB_AB"/>
</gates>
<devices>
<device name="_SMT" package="USB-AB-MICRO-SMD">
<connects>
<connect gate="G$1" pin="D+" pad="D+1"/>
<connect gate="G$1" pin="D-" pad="D-1"/>
<connect gate="G$1" pin="GND" pad="GND1"/>
<connect gate="G$1" pin="SHIELD" pad="SHLD1 SHLD2 SHLD3"/>
<connect gate="G$1" pin="USBID" pad="ID1"/>
<connect gate="G$1" pin="VBUS" pad="VBUS1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11794"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MINI_USB" prefix="J">
<gates>
<gate name="G$1" symbol="MINI_USB"/>
</gates>
<devices>
<device name="" package="UX60-MB-5ST">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5V" pad="VCC"/>
<connect gate="G$1" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ACES_LOGO">
<gates>
<gate name="G$1" symbol="LOGO"/>
</gates>
<devices>
<device name="SMALL_TSILK_TEXT" package="SMALL_TSILK_TEXT">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TINY_BSILK_TEXT" package="TINY_BSILK_TEXT">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MEDIUM_TSILK" package="MEDIUM_TSILK">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MEDIUM_TSILK_TEXT" package="MEDIUM_TSILK_TEXT">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TINY_TSILK_NO_TEXT" package="TINY_TSILK">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMALL_TSILK" package="SMALL_TSILK">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="MEDIUM_BSILK">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MEDIUM_BSILK_TEXT" package="MEDIUM_BSILK_TEXT">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMALL_BSILK" package="SMALL_BSILK">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMALL_BSILK_TEXT" package="SMALL_BSILK_TEXT">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TINY_BSILK" package="TINY_BSILK">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TINY_TSILK_TEXT" package="TINY_TSILK_TEXT">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOUNTING_HOLE">
<description>&lt;p&gt;For consistency, ACES use 3mm &lt;a href="https://www.mcmaster.com/92492a715"&gt;screws&lt;/a&gt; and &lt;a href="https://www.mcmaster.com/94180a333"&gt;heat set inserts&lt;/a&gt; from McMaster-Carr for their PCB and Case designs.&lt;/p&gt;

&lt;p&gt;These holes were ported from the microbuilder library and offer no ground protection as we typically use nylon hardware.&lt;/p&gt;
&lt;p&gt;You are encouraged to use this these mounting  holes for your PCB designs.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MOUNTING_HOLE"/>
</gates>
<devices>
<device name="" package="MOUNTINGHOLE_3.2MM_PLATEDTHIN">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
