<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<library>
<packages>
<package name="B3F-40XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="B3F-40XX-ROUND">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="6MM">
</package>
<package name="TRIM-3386">
</package>
<package name="TRIMPOT-PTH-3386U">
<description>&lt;h3&gt;Trimpot - PTH, Trimpot w/ finger-adjustable knob&lt;/h3&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/9806"&gt;Trimpot 10K with Knob&lt;/a&gt; (COM-09806)&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.sparkfun.com/datasheets/Components/General/TSR-3386.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="MEDIUM_TSILK">
</package>
<package name="CONN_SUPPLY">
<description>Digikey Information (Added 2019 03 14. C. D'Arcy)

Part #:
SAM1225-02-ND 


Description:
CONN RCPT 2POS 0.1 GOLD PCB R/A

&lt;p&gt;Created on 2019 03 18 by C. D'Arcy.&lt;/p&gt;
&lt;p&gt;&lt;img src="http://darcy.rsgc.on.ca/ACES/PCBs/images/ACESLogov2.png" align="left" width="100"&gt;&lt;/p&gt;</description>
</package>
<package name="FIXEDRESISTOR1/4W">
</package>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="CPOL-RADIAL-2.5MM-5MM">
<description>2.5 mm spaced PTHs with 5 mm diameter outline and standard solder mask</description>
</package>
<package name="CAP-PTH-2.54">
<description>2 PTH spaced 0.1" apart</description>
</package>
<package name="CPOL-RADIAL-5MM-10MM">
<description>5 mm spaced PTHs in 10 mm diameter silk ring</description>
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
<package name="LED10MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
10 mm, round</description>
</package>
<package name="TACTILE_SWITCH_PTH_6.0MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, 6.0mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.omron.com/ecb/products/pdf/en-b3f.pdf"&gt;Datasheet&lt;/a&gt; (B3F-1000)&lt;/p&gt;</description>
</package>
<package name="HDSP">
<description>&lt;b&gt;LED DISPLAY&lt;/b&gt;&lt;p&gt;
 15-mm 1 character 7 segment, decimal point right</description>
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="M251">
<description>&lt;b&gt;SLIDING SWITCH&lt;/b&gt;&lt;p&gt;
Mors, distributor Buerklin, 11G702</description>
</package>
<package name="PJ-102A">
<description>&lt;b&gt;DC POWER JACK&lt;/b&gt;
&lt;p&gt;&lt;b&gt;Digikey Part:&lt;/b&gt; &lt;a href="https://www.digikey.ca/product-detail/en/cui-devices/PJ-102A/CP-102A-ND/275425" target="_blank"&gt;CP-102A-ND&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Source: &lt;a href="https://www.cuidevices.com/product/resource/pj-102a.pdf"&gt;PJ-102A.pdf&lt;/a&gt;&lt;/p&gt;

&lt;p&gt;Modified on 2020 01 09 by C. D'Arcy to ensure rectangular-shaped milling of lead holes (&lt;b&gt;Layer 45&lt;/b&gt;).&lt;/p&gt;
&lt;p&gt;These jacks have striaght tapered pins requiring only drill holes, not necessarily milled ovals.&lt;/p&gt;
&lt;p&gt;&lt;img src="http://darcy.rsgc.on.ca/ACES/PCBs/images/ACESLogov2.png" align="left" width="100"&gt;&lt;/p&gt;</description>
</package>
<package name="LB10">
<description>&lt;B&gt;LED BLOCK&lt;/B&gt;&lt;p&gt;
10-LED bar graph, DIL, Siemens</description>
</package>
<package name="DIP28">
<description>Standard 28-pin DIP package.&lt;br&gt;
IC needs to have legs bent before insertion.</description>
</package>
<package name="DIP14">
</package>
<package name="TO220DS">
<description>&lt;b&gt;TO 220 D&lt;/b&gt; vertical (Anode1; Anode2; Gate)</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL10">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL18">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL22">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL24">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL24S">
<description>&lt;b&gt;Dual In Line Package Small&lt;/b&gt;</description>
</package>
<package name="HC49US">
<description>&lt;h3&gt;HC49/US 11.6x4.6mm PTH Crystal&lt;/h3&gt;
&lt;p&gt;&lt;a href="https://www.digikey.com/Web%20Export/Supplier%20Content/Citizen_300/PDF/Citizen_HC49US.pdf?redirected=1"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="TC38H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="78XXL">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
<package name="78LXX">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
<package name="TO92_VREG">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
<package name="2N3904">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
grid 5.08 mm</description>
</package>
<package name="TO92-TAPE">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
grid 5.08 mm</description>
</package>
<package name="P2N2222A">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
grid 5.08 mm</description>
</package>
<package name="2N2222A">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
grid 5.08 mm</description>
</package>
<package name="2N3906">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
grid 5.08 mm</description>
</package>
<package name="BC547">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
grid 5.08 mm</description>
</package>
<package name="2N4401">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
grid 5.08 mm</description>
</package>
<package name="2N4403">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
grid 5.08 mm</description>
</package>
<package name="TMP36">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
grid 5.08 mm

&lt;p&gt;Created on 2019 03 18 by C. D'Arcy.&lt;/p&gt;
&lt;p&gt;&lt;img src="http://darcy.rsgc.on.ca/ACES/PCBs/images/ACESLogov2.png" align="left" width="100"&gt;&lt;/p&gt;</description>
</package>
<package name="DO41">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
<package name="DO35">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2 mm, horizontal, grid 10.16 mm</description>
</package>
<package name="RN-9">
<description>&lt;b&gt;RESISTOR NETWORK&lt;/b&gt;</description>
</package>
<package name="RN-10">
<description>&lt;b&gt;RESISTOR NETWORK&lt;/b&gt;</description>
</package>
<package name="ICSP">
<description>&lt;h3&gt;Plated Through Hole - 2x3&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="RN-11">
<description>&lt;b&gt;RESISTOR NETWORK&lt;/b&gt;</description>
</package>
<package name="SIL8">
<description>&lt;b&gt;Single In Line&lt;/b&gt;</description>
</package>
<package name="B25X">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Beckman Helitrim 25</description>
</package>
<package name="D-10">
<description>&lt;b&gt;DIODE&lt;/b&gt;</description>
</package>
<package name="TO220">
<description>&lt;b&gt;TO 220 horizontal&lt;/b&gt;</description>
</package>
<package name="TO220AH">
<description>&lt;b&gt;Molded Package&lt;/b&gt;&lt;p&gt;
grid 2.54 mm</description>
</package>
<package name="BC557">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
grid 5.08 mm</description>
</package>
<package name="1X06/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;

&lt;p&gt;Modified on 2019 03 18 by C. D'Arcy.&lt;/p&gt;
&lt;p&gt;&lt;img src="http://darcy.rsgc.on.ca/ACES/PCBs/images/ACESLogov2.png" align="left" width="100"&gt;&lt;/p&gt;</description>
</package>
<package name="DIP16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="AUDIO_JACK">
<description>&lt;h3&gt;3.5mm Stereo Audio Jack&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Audio-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Audio_Jack&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="7-SEGMENT-4DIGIT-YOUNGSUN-LONGPADS">
</package>
<package name="SEGMENT_BL-M07C881UR">
<description>&lt;p&gt;Modified on 2019 03 18 by C. D'Arcy.&lt;/p&gt;
&lt;p&gt;&lt;img src="http://darcy.rsgc.on.ca/ACES/PCBs/images/ACESLogov2.png" align="left" width="100"&gt;&lt;/p&gt;</description>
</package>
<package name="MINI_USB">
<description>&lt;b&gt;MINI USB-B R/A DIP&lt;/b&gt;&lt;p&gt;
Source: http://www.cypressindustries.com/pdf/32005-601.pdf</description>
</package>
<package name="BATTCON_12MM_PTH">
<description>&lt;h3&gt;12mm Coin Cell Battery (CR1225) Holder - PTH&lt;/h3&gt;
&lt;p&gt;This is a through hole 12mm coin cell battery holder. Holds battery in place with friction. Metal housing is +, PCB pad underneath is -.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Prototyping/KEY-3001.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;

&lt;p&gt;Modified on 2019 03 18 by C. D'Arcy.&lt;/p&gt;
&lt;p&gt;&lt;img src="http://darcy.rsgc.on.ca/ACES/PCBs/images/ACESLogov2.png" align="left" width="100"&gt;&lt;/p&gt;</description>
</package>
<package name="LED_RGB_CA">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Created on 2019 03 18 by C. D'Arcy.&lt;/p&gt;
&lt;p&gt;&lt;img src="http://darcy.rsgc.on.ca/ACES/PCBs/images/ACESLogov2.png" align="left" width="100"&gt;&lt;/p&gt;</description>
</package>
<package name="LED_RGB_CC">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Created on 2019 03 18 by C. D'Arcy.&lt;/p&gt;
&lt;p&gt;&lt;img src="http://darcy.rsgc.on.ca/ACES/PCBs/images/ACESLogov2.png" align="left" width="100"&gt;&lt;/p&gt;</description>
</package>
<package name="BOURNS_3352P">
<description>&lt;b&gt;3/8" Round Thumbwheel Potentiometer&lt;/b&gt;
&lt;p&gt;Designed for &lt;b&gt;RSGC ACES&lt;/b&gt; from dimensions found in this &lt;a href="https://www.bourns.com/docs/Product-Datasheets/3352.pdf"&gt;datasheet&lt;/a&gt;.&lt;/p&gt;
Created on 2019 03 18 by C. D'Arcy.&lt;br&gt;
&lt;p&gt;&lt;img src="http://darcy.rsgc.on.ca/ACES/PCBs/images/ACESLogov2.png" align="left" width="100"&gt;&lt;/p&gt;</description>
</package>
<package name="RESONATOR-PTH-7.6X3.8">
<description>&lt;h3&gt;7.6x3.8mm 3-Pin PTH Resonator&lt;/h3&gt;
&lt;p&gt;0.1" pitch&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/Resonator-16MHz.pdf"&gt;Example datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="TDA7052A">
<description>&lt;p&gt;Created on 2019 03 18 by C. D'Arcy.&lt;/p&gt;
&lt;p&gt;&lt;img src="http://darcy.rsgc.on.ca/ACES/PCBs/images/ACESLogov2.png" align="left" width="100"&gt;&lt;/p&gt;</description>
</package>
<package name="LCD1602">
<description>Source: &lt;b&gt;Adafruit Library: &lt;/b&gt;HD77780LCD

&lt;p&gt;Modified on 2019 03 18 by C. D'Arcy to include RSGC ACES Greeting!&lt;/p&gt;
&lt;p&gt;&lt;img src="http://darcy.rsgc.on.ca/ACES/PCBs/images/ACESLogov2.png" align="left" width="100"&gt;&lt;/p&gt;</description>
</package>
<package name="SMALL_TSILK">
</package>
<package name="MOUNTINGHOLE_3.2MM_PLATEDTHIN">
</package>
<package name="MEDIUM_BSILK">
</package>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="MEDIUM_TSILK_TEXT">
</package>
<package name="MEDIUM_BSILK_TEXT">
</package>
<package name="SMALL_TSILK_TEXT">
</package>
<package name="SMALL_BSILK">
</package>
<package name="SMALL_BSILK_TEXT">
</package>
<package name="SIL9">
<description>&lt;b&gt;Single In Line&lt;/b&gt;</description>
</package>
<package name="EG1218">
</package>
<package name="DUAL_CC_14-SEGMENT">
<description>&lt;b&gt;30.48mm(1.2 INCH) 16 SEGMENT SINGLE DIGIT ALPHANUMERIC NUMERIC DISPLAY&lt;/b&gt;
Source: PSA12-11EWA(Ver1189413040.8).pdf</description>
</package>
<package name="PJ-202AH">
<description>&lt;b&gt;DC POWER JACK&lt;/b&gt;
&lt;p&gt;&lt;b&gt;Digikey Part:&lt;/b&gt; &lt;a href="https://www.digikey.ca/product-detail/en/cui-devices/PJ-202AH/CP-202AH-ND/408450" target="_blank"&gt;CP-202AH-ND&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Source: &lt;a href="https://www.cuidevices.com/product/resource/pj-202ah.pdf"&gt;PJ-202AH.pdf&lt;/a&gt;&lt;/p&gt;

&lt;p&gt;Modified on 2020 01 09 by C. D'Arcy to ensure rectangular-shaped milling of lead holes (&lt;b&gt;Layer 45&lt;/b&gt;).&lt;/p&gt;
&lt;p&gt;These jacks have kinked pins. Hopefully I've got the milled openings correctly sized and positioned&lt;/p&gt;
&lt;p&gt;&lt;img src="http://darcy.rsgc.on.ca/ACES/PCBs/images/ACESLogov2.png" align="left" width="100"&gt;&lt;/p&gt;</description>
</package>
<package name="CAUTION_ELECTRIC">
</package>
<package name="TO220V">
<description>&lt;b&gt;TO 200 vertical&lt;/b&gt;</description>
</package>
<package name="AUDIO_JACK_SWITCHCRAFT">
<description>&lt;h3&gt;3.5mm Stereo Audio Jack&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Audio-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Audio_Jack&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
<symbols>
<symbol name="LOGO">
<description>&lt;p&gt;Created on 2019 03 18 by C. D'Arcy.&lt;/p&gt;
&lt;p&gt;&lt;img src="http://darcy.rsgc.on.ca/ACES/PCBs/images/ACESLogov2.png" align="left" width="100"&gt;&lt;/p&gt;</description>
</symbol>
<symbol name="TS2">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="P1" direction="pas"/>
</symbol>
<symbol name="TRIM-1">
<description>&lt;p&gt;Modified on 2019 03 18 by C. D'Arcy.&lt;/p&gt;
&lt;p&gt;&lt;img src="http://darcy.rsgc.on.ca/ACES/PCBs/images/ACESLogov2.png" align="left" width="100"&gt;&lt;/p&gt;</description>
<pin name="A" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="CONN_SUPPLY">
<pin name="-" direction="pas"/>
<pin name="+" direction="pas"/>
</symbol>
<symbol name="R-US">
<description>&lt;p&gt;Modified on 2019 03 18 by C. D'Arcy.&lt;/p&gt;
&lt;p&gt;&lt;img src="http://darcy.rsgc.on.ca/ACES/PCBs/images/ACESLogov2.png" align="left" width="100"&gt;&lt;/p&gt;</description>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="CAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="CAP_POL">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="LED">
<description>&lt;h3&gt;LED&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;</description>
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="SPST">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="HD7-K">
<pin name="G" direction="pas"/>
<pin name="F" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="CC@1" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="DP" direction="pas"/>
<pin name="CC" direction="pas"/>
</symbol>
<symbol name="NE555">
<pin name="TRE" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="DIS" direction="in"/>
<pin name="TRI" direction="in"/>
<pin name="VCC+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="CON" direction="in"/>
<pin name="/RES" direction="in"/>
</symbol>
<symbol name="TOGGLE">
<description>&lt;h3&gt;Single Pole, Double Throw (SPDT) Switch&lt;/h3&gt;
&lt;p&gt;Single-pole, double-throw (SPDT) switch.&lt;/p&gt;</description>
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="DC-JACK-SWITCH">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="BARGRAPH">
<description>&lt;h3&gt;LED&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;</description>
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="C1" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="C3" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="C4" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="C5" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="C6" direction="pas"/>
<pin name="A6" direction="pas"/>
<pin name="C7" direction="pas"/>
<pin name="A7" direction="pas"/>
<pin name="C8" direction="pas"/>
<pin name="A8" direction="pas"/>
<pin name="C9" direction="pas"/>
<pin name="A9" direction="pas"/>
</symbol>
<symbol name="ATMEGAXX8-28PIN">
<description>Symbol for Atmega328/168/88/48 chips, 28-pin versions</description>
<pin name="PB5(SCK)"/>
<pin name="PB7(XTAL2/TOSC2)"/>
<pin name="PB6(XTAL1/TOSC1)"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="VCC"/>
<pin name="AREF"/>
<pin name="AVCC"/>
<pin name="PB4(MISO)"/>
<pin name="PB3(MOSI/OC2)"/>
<pin name="PB2(SS/OC1B)"/>
<pin name="PB1(OC1A)"/>
<pin name="PB0(ICP)"/>
<pin name="PD7(AIN1)"/>
<pin name="PD6(AIN0)"/>
<pin name="PD5(T1)"/>
<pin name="PD4(XCK/T0)"/>
<pin name="PD3(INT1)"/>
<pin name="PD2(INT0)"/>
<pin name="PD1(TXD)"/>
<pin name="PD0(RXD)"/>
<pin name="PC5(ADC5/SCL)"/>
<pin name="PC4(ADC4/SDA)"/>
<pin name="PC3(ADC3)"/>
<pin name="PC2(ADC2)"/>
<pin name="PC1(ADC1)"/>
<pin name="PC0(ADC0)"/>
<pin name="PC6(/RESET)" function="dot"/>
</symbol>
<symbol name="ATTINY84">
<pin name="VCC" direction="pwr"/>
<pin name="(PCINT3/T0/ADC3)PA3"/>
<pin name="(PCINT2/AIN1/ADC2)PA2"/>
<pin name="(PCINT1/AIN0/ADC1)PA1"/>
<pin name="(PCINT0/AREF/ADC0)PA0"/>
<pin name="(PCINT4/T1/SCL/USCK/ADC4)PA4"/>
<pin name="(PCINT5/OC1B/MISO/DO/ADC5)PA5"/>
<pin name="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6"/>
<pin name="(PCINT7/ICP/OC0B/ADC7)PA7"/>
<pin name="(PCINT8/XTAL1/CLKI)PB0"/>
<pin name="(PCINT9/XTAL2)PB1"/>
<pin name="(PCINT10/INT0/OC0A/CKOUT)PB2"/>
<pin name="(PCINT11/~RESET/DW)PB3"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="CRYSTAL">
<description>&lt;h3&gt;Crystal (no ground pin)&lt;/h3&gt;</description>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="DS1307">
<description>&lt;h3&gt;Maxim DS1307 - I2C Real-time clock (RTC)&lt;/h3&gt;</description>
<pin name="X1"/>
<pin name="X2"/>
<pin name="VBATT"/>
<pin name="GND"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="SQW"/>
<pin name="VCC"/>
</symbol>
<symbol name="DS1307-1">
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="GND" direction="pwr"/>
<pin name="VBAT" direction="pwr"/>
<pin name="SQW/OUT"/>
<pin name="VCC" direction="pwr"/>
<pin name="X1" direction="pas"/>
<pin name="X2" direction="pas"/>
</symbol>
<symbol name="Q1">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="78XXL">
<pin name="IN" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="OUT" direction="pas"/>
</symbol>
<symbol name="78LXX">
<pin name="IN" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="OUT" direction="pas"/>
</symbol>
<symbol name="NPN">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="PNP">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="TMP36">
<description>&lt;h3&gt;TMP36 Precision Analog &amp;deg;C Temperature Sensor&lt;/h3&gt;
&lt;p&gt;The TMP36 is a low voltage, precision centigrade temperature sensor. It provides a voltage output that is linearly proportional to the Celsius temperature. It also doesn’t require any external calibration to provide typical accuracies of ±1°C at +25°C and ±2°C over the −40°C to +125°C temperature range. We like it because it’s so easy to use: Just give the device a ground and 2.7 to 5.5 VDC and read the voltage on the Vout pin. The output voltage can be converted to temperature easily using the scale factor of 10 mV/°C.&lt;/p&gt;
&lt;p&gt;Modifed on 2019 03 18 by C. D'Arcy.&lt;/p&gt;
&lt;p&gt;&lt;img src="http://darcy.rsgc.on.ca/ACES/PCBs/images/ACESLogov2.png" align="left" width="100"&gt;&lt;/p&gt;</description>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="VOUT"/>
</symbol>
<symbol name="DIODE">
<description>&lt;p&gt;Modified on 2019 03 18 by C. D'Arcy.&lt;/p&gt;
&lt;p&gt;&lt;img src="http://darcy.rsgc.on.ca/ACES/PCBs/images/ACESLogov2.png" align="left" width="100"&gt;&lt;/p&gt;</description>
<pin name="A"/>
<pin name="C"/>
</symbol>
<symbol name="RN1X9">
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="RN09">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="PINH2X3">
<description>&lt;p&gt;Created on 2019 03 18 by C. D'Arcy.&lt;/p&gt;
&lt;p&gt;&lt;img src="http://darcy.rsgc.on.ca/ACES/PCBs/images/ACESLogov2.png" align="left" width="100"&gt;&lt;/p&gt;</description>
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="ICSP">
<description>&lt;p&gt;Created on 2019 03 18 by C. D'Arcy.&lt;/p&gt;
&lt;p&gt;&lt;img src="http://darcy.rsgc.on.ca/ACES/PCBs/images/ACESLogov2.png" align="left" width="100"&gt;&lt;/p&gt;</description>
<pin name="GND" direction="pwr"/>
<pin name="RST" direction="pas"/>
<pin name="MOSI" direction="pas"/>
<pin name="SCK" direction="pas"/>
<pin name="5V" direction="pwr"/>
<pin name="MISO" direction="pas"/>
</symbol>
<symbol name="RN10">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="RNV">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="PUSHBUTTON">
<pin name="P$1" direction="pas"/>
<pin name="P$2" direction="pas"/>
</symbol>
<symbol name="5-I/O-1">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="PB4"/>
<pin name="(CLOCK)PB3"/>
<pin name="(SCK)PB2"/>
<pin name="(MISO)PB1"/>
<pin name="(MOSI)PB0"/>
</symbol>
<symbol name="ATTINY85">
<pin name="PB5/PCINT5/!RESET!/ADC0/DW"/>
<pin name="PB3/PCINT3/CLKI/ADC3"/>
<pin name="PB4/PCINT4/ADC2"/>
<pin name="PB0/PCINT0/AIN0/OC0A/MOSI" direction="pas"/>
<pin name="PB1/PCINT1/AIN1/OC0B/INT0/MISO"/>
<pin name="PB2/PCINT2/SCK/ADC1/T0"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="N-MOSFET">
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="IGFET-EN-GDS">
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
</symbol>
<symbol name="N-DAR">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="ULN2803">
<description>&lt;p&gt;Created on 2019 03 18 by C. D'Arcy.&lt;/p&gt;
&lt;p&gt;&lt;img src="http://darcy.rsgc.on.ca/ACES/PCBs/images/ACESLogov2.png" align="left" width="100"&gt;&lt;/p&gt;</description>
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
</symbol>
<symbol name="ULN2003">
<description>&lt;p&gt;Created on 2019 03 18 by C. D'Arcy.&lt;/p&gt;
&lt;p&gt;&lt;img src="http://darcy.rsgc.on.ca/ACES/PCBs/images/ACESLogov2.png" align="left" width="100"&gt;&lt;/p&gt;</description>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="COM" direction="pas"/>
<pin name="OUT7" direction="out"/>
<pin name="OUT6" direction="out"/>
<pin name="OUT5" direction="out"/>
<pin name="OUT4" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT1" direction="out"/>
</symbol>
<symbol name="MSGEQ7">
<pin name="CLKIN"/>
<pin name="GND"/>
<pin name="RESET"/>
<pin name="IN"/>
<pin name="STROBE" direction="in"/>
<pin name="OUT" direction="in"/>
<pin name="VSS(GND)" direction="in"/>
<pin name="VDD" direction="in"/>
</symbol>
<symbol name="PINHD6">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="74595">
<pin name="QB" direction="hiz"/>
<pin name="QC" direction="hiz"/>
<pin name="QD" direction="hiz"/>
<pin name="QE" direction="hiz"/>
<pin name="QF" direction="hiz"/>
<pin name="QG" direction="hiz"/>
<pin name="QH" direction="hiz"/>
<pin name="MR" direction="in" function="dot"/>
<pin name="LATCH" direction="in" function="clk"/>
<pin name="CLOCK" direction="in" function="clk"/>
<pin name="OE" direction="in" function="dot"/>
<pin name="DATA" direction="in"/>
<pin name="QA" direction="hiz"/>
<pin name="QH*" direction="hiz"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="AUDIO_JACK">
<description>&lt;h3&gt; Audio Jack &lt;/h3&gt;
&lt;p&gt;  Basic Audio Jack with bypass switches&lt;/p&gt;</description>
<pin name="RING"/>
<pin name="TIP"/>
<pin name="GND" direction="pwr"/>
<pin name="NP"/>
<pin name="TIP_SWITCH"/>
</symbol>
<symbol name="7-SEGMENT-4DIGIT-YOUNGSUN">
<pin name="DIG2"/>
<pin name="DIG3"/>
<pin name="DIG4"/>
<pin name="COL-A"/>
<pin name="APOS-A"/>
<pin name="A"/>
<pin name="B"/>
<pin name="C"/>
<pin name="D"/>
<pin name="E"/>
<pin name="F"/>
<pin name="G"/>
<pin name="DP"/>
<pin name="COL-C"/>
<pin name="APOS-C"/>
<pin name="DIG1"/>
</symbol>
<symbol name="SEGMENT_8X8_CATHODEROW">
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="K1"/>
<pin name="K2"/>
<pin name="K3"/>
<pin name="K4"/>
<pin name="K5"/>
<pin name="K6"/>
<pin name="K7"/>
<pin name="K8"/>
</symbol>
<symbol name="MINI-USB-5">
<pin name="VIN" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="SHIELD2">
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
</symbol>
<symbol name="BATTERY">
<description>&lt;h3&gt;Battery (Single-Cell)&lt;/h3&gt;</description>
<pin name="-" direction="pwr"/>
<pin name="+" direction="pwr"/>
</symbol>
<symbol name="TPIC6C595">
<description>&lt;p&gt;Created on 2019 03 18 by C. D'Arcy.&lt;/p&gt;
&lt;p&gt;&lt;img src="http://darcy.rsgc.on.ca/ACES/PCBs/images/ACESLogov2.png" align="left" width="100"&gt;&lt;/p&gt;</description>
<pin name="DRAIN1" direction="in"/>
<pin name="DRAIN2" direction="in"/>
<pin name="DRAIN3" direction="in"/>
<pin name="DRAIN4" direction="in"/>
<pin name="DRAIN5" direction="in"/>
<pin name="DRAIN6" direction="in"/>
<pin name="DRAIN7" direction="in"/>
<pin name="SCL" direction="in" function="dot"/>
<pin name="SCK" direction="in" function="clk"/>
<pin name="RCK" direction="in" function="clk"/>
<pin name="/CLR" direction="in" function="dot"/>
<pin name="SER_IN" direction="in"/>
<pin name="DRAIN0" direction="in"/>
<pin name="SER_OUT" direction="hiz"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="LED-RGB-CA">
<description>&lt;h3&gt;RGB LED - Common Anode&lt;/h3&gt;
&lt;p&gt;4 pin Common Anode RGB LED&lt;/p&gt;
&lt;p&gt;Modified on 2019 03 18 by C. D'Arcy.&lt;/p&gt;
&lt;p&gt;&lt;img src="http://darcy.rsgc.on.ca/ACES/PCBs/images/ACESLogov2.png" align="left" width="100"&gt;&lt;/p&gt;</description>
<pin name="GRN"/>
<pin name="BLU"/>
<pin name="A"/>
<pin name="RED"/>
</symbol>
<symbol name="LED-RGB-CC">
<description>&lt;h3&gt;RGB LED - Common Cathode&lt;/h3&gt;
&lt;p&gt;4 pin Common Cathode RGB LED&lt;/p&gt;
&lt;p&gt;Modified on 2019 03 18 by C. D'Arcy.&lt;/p&gt;
&lt;p&gt;&lt;img src="http://darcy.rsgc.on.ca/ACES/PCBs/images/ACESLogov2.png" align="left" width="100"&gt;&lt;/p&gt;</description>
<pin name="GRN"/>
<pin name="BLU"/>
<pin name="C"/>
<pin name="RED"/>
</symbol>
<symbol name="RESONATOR">
<description>&lt;h3&gt;Resonator&lt;/h3&gt;</description>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="TDA7052A">
<pin name="OUT-"/>
<pin name="GND2"/>
<pin name="NC" direction="nc"/>
<pin name="OUT+"/>
<pin name="NC4" direction="nc"/>
<pin name="GND1" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="VP" direction="in"/>
</symbol>
<symbol name="CLCD">
<pin name="K" direction="in"/>
<pin name="A" direction="in"/>
<pin name="DB7"/>
<pin name="DB6"/>
<pin name="DB5"/>
<pin name="DB4"/>
<pin name="DB3"/>
<pin name="DB2"/>
<pin name="DB1"/>
<pin name="DB0"/>
<pin name="E" direction="in"/>
<pin name="RW" direction="in"/>
<pin name="RS" direction="in"/>
<pin name="VO" direction="in"/>
<pin name="VDD" direction="sup"/>
<pin name="VSS" direction="sup"/>
</symbol>
<symbol name="HD7-A">
<pin name="DP" direction="pas"/>
<pin name="F" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="CA" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="Z" direction="pas"/>
<pin name="CA@1" direction="pas"/>
</symbol>
<symbol name="MOUNTING_HOLE">
</symbol>
<symbol name="ADC0804">
<pin name="DB0" direction="in"/>
<pin name="DB1" direction="in"/>
<pin name="DB2" direction="in"/>
<pin name="DB3" direction="in"/>
<pin name="DB4" direction="in"/>
<pin name="DB5" direction="in"/>
<pin name="DB6" direction="in"/>
<pin name="DB7" direction="in"/>
<pin name="DGND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="/CS" direction="in" function="dot"/>
<pin name="/RD" direction="in" function="dot"/>
<pin name="/WR" direction="in" function="dot"/>
<pin name="/INTR" direction="in" function="dot"/>
<pin name="CLK_IN" direction="in" function="clk"/>
<pin name="AGND" direction="pwr"/>
<pin name="VREF/2" direction="in"/>
<pin name="VIN+" direction="pwr"/>
<pin name="VIN-" direction="pwr"/>
<pin name="CLK_R" direction="in" function="clk"/>
</symbol>
<symbol name="HD7">
<pin name="DP" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="F" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="S8" direction="pwr"/>
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="S3" direction="pwr"/>
</symbol>
<symbol name="RN08">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="AT28C16">
<pin name="A7" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="!CE" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="!WE" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A8" direction="in"/>
</symbol>
<symbol name="2816">
<pin name="A7" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="!CE" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="!WE" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A8" direction="in"/>
</symbol>
<symbol name="PWRN">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="+5V">
<pin name="+5V" direction="sup"/>
</symbol>
<symbol name="VCC">
<pin name="VCC" direction="sup"/>
</symbol>
<symbol name="16-SEG-LED-A">
<pin name="A" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="F" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="H" direction="pas"/>
<pin name="K" direction="pas"/>
<pin name="M" direction="pas"/>
<pin name="N" direction="pas"/>
<pin name="P" direction="pas"/>
<pin name="R" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="T" direction="pas"/>
<pin name="U" direction="pas"/>
<pin name="DP" direction="pas"/>
<pin name="AN" direction="pas"/>
</symbol>
<symbol name="14-SEG-LED-A">
<pin name="A" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="F" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="H" direction="pas"/>
<pin name="K" direction="pas"/>
<pin name="M" direction="pas"/>
<pin name="N" direction="pas"/>
<pin name="P" direction="pas"/>
<pin name="R" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="T" direction="pas"/>
<pin name="U" direction="pas"/>
<pin name="DP" direction="pas"/>
<pin name="AN" direction="pas"/>
</symbol>
<symbol name="14-SEG-LED-DUAL-C">
<pin name="A" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="F" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="H" direction="pas"/>
<pin name="J" direction="pas"/>
<pin name="K" direction="pas"/>
<pin name="L" direction="pas"/>
<pin name="M" direction="pas"/>
<pin name="N" direction="pas"/>
<pin name="P" direction="pas"/>
<pin name="DP" direction="pas"/>
<pin name="CC1" direction="pas"/>
<pin name="CC2" direction="pas"/>
</symbol>
<symbol name="SIS">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="AUDIO_JACK_SWITCHCRAFT">
<description>&lt;h3&gt; Switchcraft Audio Jack &lt;/h3&gt;
&lt;h3&gt;3.5mm Stereo Audio Jack&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Audio-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Audio_Jack&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<pin name="RING"/>
<pin name="TIP"/>
<pin name="GND" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ACES_LOGO">
<description>&lt;b&gt;Required for use&lt;/b&gt; on your boards if ACES budget is paying for your order.</description>
<gates>
<gate name="G$1" symbol="LOGO"/>
</gates>
<devices>
<device name="MEDIUM_TSILK" package="MEDIUM_TSILK">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMALL" package="SMALL_TSILK">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="MEDIUM_BSILK">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MEDIUM_BSILK_TEXT" package="MEDIUM_BSILK_TEXT">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MEDIUM_TSILK_TEXT" package="MEDIUM_TSILK_TEXT">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMALL_TSILK_TEXT" package="SMALL_TSILK_TEXT">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMALL_BSILK" package="SMALL_BSILK">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMALL_BSILK_TEXT" package="SMALL_BSILK_TEXT">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOMENTARY_BUTTONS" prefix="S" uservalue="yes">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="TS2"/>
</gates>
<devices>
<device name="" package="B3F-40XX">
<connects>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="P1" pad="4"/>
<connect gate="1" pin="S" pad="1"/>
<connect gate="1" pin="S1" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="OMRON COMPONENTS USA"/>
<attribute name="MPN" value="B3F-4000"/>
<attribute name="OC_FARNELL" value="176434"/>
<attribute name="OC_NEWARK" value="36K3105"/>
</technology>
</technologies>
</device>
<device name="-ROUND" package="B3F-40XX-ROUND">
<connects>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="P1" pad="4"/>
<connect gate="1" pin="S" pad="1"/>
<connect gate="1" pin="S1" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="6MMSMALL" package="TACTILE_SWITCH_PTH_6.0MM">
<connects>
<connect gate="1" pin="P" pad="1"/>
<connect gate="1" pin="P1" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
<connect gate="1" pin="S1" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRIMPOT" prefix="R" uservalue="yes">
<description>See &lt;b&gt;pot&lt;/b&gt; library for more 'European?' smaller options.

&lt;p&gt;Modified on 2019 03 18 by C. D'Arcy.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TRIM-1"/>
</gates>
<devices>
<device name="BLUE_ONE" package="TRIM-3386">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="B" pad="3"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMALLER" package="6MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="E"/>
<connect gate="G$1" pin="C" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="TRIMPOT-PTH-3386U">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="B" pad="3"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BECKMAN25" package="B25X">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BOURNS_3352P" package="BOURNS_3352P">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_SUPPLY" prefix="H">
<description>&lt;p&gt;&lt;b&gt;Digikey Part #:&lt;/b&gt; &lt;a href="https://www.digikey.ca/product-detail/en/samtec-inc/SSW-102-02-G-S-RA/SAM1225-02-ND/1112501"&gt;SAM1225-02-ND&lt;/a&gt;&lt;/p&gt;

Used, typically, for external power supply wires to a PCB or Appliance.

&lt;p&gt;&lt;b&gt;Last Ordered: &lt;/b&gt;2019 02 07&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CONN_SUPPLY"/>
</gates>
<devices>
<device name="" package="CONN_SUPPLY">
<connects>
<connect gate="G$1" pin="+" pad="VCC"/>
<connect gate="G$1" pin="-" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESISTOR" prefix="R">
<description>Based on rcl Libray part R-US_0207/10 with longer oval pads for easier hand soldering.
&lt;p&gt;&lt;strong&gt;Digikey&lt;/strong&gt;&lt;/p&gt;

&lt;b&gt;Part #:&lt;/b&gt; &lt;a href="https://www.digikey.ca/products/en/resistors/through-hole-resistors/53?k=fixed+resistor&amp;k=&amp;pkeyword=fixed+resistor&amp;sv=1&amp;pv2=4&amp;pv174=18&amp;sf=0&amp;FV=ffe00035%2Cfffc000d%2C1c0003%2C1f140000%2Cmu470+Ohms%7C2085&amp;quantity=&amp;ColumnSort=0&amp;page=1&amp;stock=1&amp;pageSize=25"&gt;470QBK-ND&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="" package="0207/10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP_DISK" prefix="C">
<description>Use for 0.1&amp;mu;F (103) and 0.01&amp;mu;F (104).

&lt;p&gt;Also suitable for 22&amp;rho;F crystal filter caps for offboard &lt;b&gt;ATmega328p&lt;/b&gt;.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="" package="CAP-PTH-2.54">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAPACITOR_POLARIZED" prefix="C">
<gates>
<gate name="G$1" symbol="CAP_POL"/>
</gates>
<devices>
<device name="" package="CPOL-RADIAL-2.5MM-5MM">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LARGE" package="CPOL-RADIAL-5MM-10MM">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED" prefix="L">
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="5MM" package="LED5MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="10MM" package="LED10MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3MM" package="LED3MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="555" prefix="IC">
<description>Check out this &lt;b&gt;&lt;a href="https://www.allaboutcircuits.com/tools/555-timer-astable-circuit/"&gt;online 555 calculator&lt;/a&gt;&lt;/b&gt; for desired RC combinations.</description>
<gates>
<gate name="G$1" symbol="NE555"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="/RES" pad="4"/>
<connect gate="G$1" pin="CON" pad="5"/>
<connect gate="G$1" pin="DIS" pad="7"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="TRE" pad="6"/>
<connect gate="G$1" pin="TRI" pad="2"/>
<connect gate="G$1" pin="VCC+" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SLIDE_SWITCH" prefix="S">
<gates>
<gate name="G$1" symbol="TOGGLE"/>
</gates>
<devices>
<device name="" package="M251">
<connects>
<connect gate="G$1" pin="O" pad="1"/>
<connect gate="G$1" pin="P" pad="2"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EG1218" package="EG1218">
<connects>
<connect gate="G$1" pin="O" pad="O"/>
<connect gate="G$1" pin="P" pad="P"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DC_JACK" prefix="J">
<description>Through hole pins are either tapered pins (PJ-102A) or eyelet (&lt;em&gt;straight or kinked&lt;/em&gt;) PJ-202AH.</description>
<gates>
<gate name="G$1" symbol="DC-JACK-SWITCH"/>
</gates>
<devices>
<device name="/PJ-102A" package="PJ-102A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/PJ-202AH" package="PJ-202AH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BARGRAPH" prefix="L">
<description>&lt;p&gt;&lt;b&gt;Digikey Part #'s:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.digikey.ca/product-detail/en/everlight-electronics-co-ltd/MV54164/1080-1183-ND/2675674"&gt;1080-1183-ND (Green)&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.digikey.ca/product-detail/en/lite-on-inc/LTA-1000HR/160-1066-ND/153273"&gt;160-1066-ND (Red)&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.digikey.ca/product-detail/en/lite-on-inc/LTA-1000Y/160-1068-ND/153283"&gt;160-1068-ND  (Yellow)&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.digikey.ca/products/en/optoelectronics/leds-circuit-board-indicators-arrays-light-bars-bar-graphs/106?k=&amp;pkeyword=&amp;sv=1&amp;pv1989=0&amp;pv37=1671&amp;sf=0&amp;FV=ffe0006a&amp;quantity=&amp;ColumnSort=0&amp;page=1&amp;stock=1&amp;pageSize=25"&gt;1497-1079-5-ND  (Blue)&lt;/a&gt;*&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
* pricey!

&lt;p&gt;&lt;b&gt;Last Ordered:&lt;/b&gt; 2019 02 28&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BARGRAPH"/>
</gates>
<devices>
<device name="" package="LB10">
<connects>
<connect gate="G$1" pin="A" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="2"/>
<connect gate="G$1" pin="A9" pad="1"/>
<connect gate="G$1" pin="C" pad="11"/>
<connect gate="G$1" pin="C1" pad="12"/>
<connect gate="G$1" pin="C2" pad="13"/>
<connect gate="G$1" pin="C3" pad="14"/>
<connect gate="G$1" pin="C4" pad="15"/>
<connect gate="G$1" pin="C5" pad="16"/>
<connect gate="G$1" pin="C6" pad="17"/>
<connect gate="G$1" pin="C7" pad="18"/>
<connect gate="G$1" pin="C8" pad="19"/>
<connect gate="G$1" pin="C9" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA328P_PDIP" prefix="MCU">
<description>&lt;h3&gt;Atmel 328P&lt;/h3&gt;
&lt;p&gt;Through hole ATMEGA328P&lt;br&gt;
uC used in the Arduino:
32kb flash, 1k EEPROM, 2k SRAM&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.sparkfun.com/datasheets/Components/SMD/ATMega328.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Use together with either the &lt;b&gt;CRYSTAL_16MHz&lt;/b&gt; or &lt;b&gt;RESONATOR&lt;/b&gt; in this library.&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="ATMEGAXX8-28PIN"/>
</gates>
<devices>
<device name="" package="DIP28">
<connects>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="GND@2" pad="22"/>
<connect gate="G$1" pin="PB0(ICP)" pad="14"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="15"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="16"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="17"/>
<connect gate="G$1" pin="PB4(MISO)" pad="18"/>
<connect gate="G$1" pin="PB5(SCK)" pad="19"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="9"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="10"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="1"/>
<connect gate="G$1" pin="PD0(RXD)" pad="2"/>
<connect gate="G$1" pin="PD1(TXD)" pad="3"/>
<connect gate="G$1" pin="PD2(INT0)" pad="4"/>
<connect gate="G$1" pin="PD3(INT1)" pad="5"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="6"/>
<connect gate="G$1" pin="PD5(T1)" pad="11"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="12"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="13"/>
<connect gate="G$1" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09136"/>
<attribute name="VALUE" value="328P"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY84" prefix="MCU">
<gates>
<gate name="G$1" symbol="ATTINY84"/>
</gates>
<devices>
<device name="" package="DIP14">
<connects>
<connect gate="G$1" pin="(PCINT0/AREF/ADC0)PA0" pad="13"/>
<connect gate="G$1" pin="(PCINT1/AIN0/ADC1)PA1" pad="12"/>
<connect gate="G$1" pin="(PCINT10/INT0/OC0A/CKOUT)PB2" pad="5"/>
<connect gate="G$1" pin="(PCINT11/~RESET/DW)PB3" pad="4"/>
<connect gate="G$1" pin="(PCINT2/AIN1/ADC2)PA2" pad="11"/>
<connect gate="G$1" pin="(PCINT3/T0/ADC3)PA3" pad="10"/>
<connect gate="G$1" pin="(PCINT4/T1/SCL/USCK/ADC4)PA4" pad="9"/>
<connect gate="G$1" pin="(PCINT5/OC1B/MISO/DO/ADC5)PA5" pad="8"/>
<connect gate="G$1" pin="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6" pad="7"/>
<connect gate="G$1" pin="(PCINT7/ICP/OC0B/ADC7)PA7" pad="6"/>
<connect gate="G$1" pin="(PCINT8/XTAL1/CLKI)PB0" pad="2"/>
<connect gate="G$1" pin="(PCINT9/XTAL2)PB1" pad="3"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CRYSTAL_16MHZ" prefix="X">
<gates>
<gate name="G$1" symbol="CRYSTAL"/>
</gates>
<devices>
<device name="" package="HC49US">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS1307" prefix="IC">
<description>&lt;b&gt;DS1307&lt;/b&gt;
&lt;p&gt;
Real time clock (RTC) with battery backup ability. Talk to it via i2c</description>
<gates>
<gate name="G$1" symbol="DS1307-1"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="SQW/OUT" pad="7"/>
<connect gate="G$1" pin="VBAT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="X1" pad="1"/>
<connect gate="G$1" pin="X2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CRYSTAL_32.768KHZ" prefix="X">
<description>&lt;p&gt;&lt;b&gt;Digikey Part #:&lt;/b&gt;  &lt;a href="https://www.digikey.ca/product-detail/en/abracon-llc/AB38T-32.768KHZ/535-9034-ND/675229"&gt;535-9034-ND&lt;/a&gt;&lt;/p&gt;

&lt;p&gt;&lt;b&gt;Last Ordered:&lt;/b&gt; 2019 01 07&lt;/p&gt;

Used for DS1307 RTCs.</description>
<gates>
<gate name="G$1" symbol="CRYSTAL"/>
</gates>
<devices>
<device name="" package="TC38H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM78XX" prefix="IC" uservalue="yes">
<description>&lt;b&gt;1+ A Positive Voltage Regulators&lt;/b&gt;
&lt;p&gt;5V Example: &lt;b&gt;&lt;a href="https://media.digikey.com/pdf/Data%20Sheets/ON%20Semiconductor%20PDFs/MC7800(A,AE),NCV7800.pdf"&gt;LM7805&lt;/a&gt;&lt;/p&gt;</description>
<gates>
<gate name="A" symbol="78XXL"/>
</gates>
<devices>
<device name="" package="78XXL">
<connects>
<connect gate="A" pin="GND" pad="GND"/>
<connect gate="A" pin="IN" pad="IN"/>
<connect gate="A" pin="OUT" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="78LXX" prefix="IC">
<description>&lt;b&gt;100mA Fixed Output Linear Regulator&lt;/b&gt;

&lt;p&gt;5V Example: &lt;b&gt;&lt;a href="http://www.ti.com.cn/cn/lit/ds/symlink/lm78l.pdf"&gt;78L05&lt;/a&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="78LXX"/>
</gates>
<devices>
<device name="" package="TO92-TAPE">
<connects>
<connect gate="G$1" pin="GND" pad="B"/>
<connect gate="G$1" pin="IN" pad="C"/>
<connect gate="G$1" pin="OUT" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NPN" prefix="Q">
<description>&lt;b&gt;NPN TRANSISTOR&lt;/b&gt;
Big oval pads</description>
<gates>
<gate name="G$1" symbol="NPN"/>
</gates>
<devices>
<device name="2N3904" package="2N3904">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P2N2222A" package="P2N2222A">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2N2222A" package="2N2222A">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BC547" package="BC547">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2N4401" package="2N4401">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PNP" prefix="Q">
<gates>
<gate name="G$1" symbol="PNP"/>
</gates>
<devices>
<device name="2N3906" package="2N3906">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2N4403" package="2N4403">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BC547" package="BC557">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TMP36" prefix="IC">
<gates>
<gate name="G$1" symbol="TMP36"/>
</gates>
<devices>
<device name="" package="TMP36">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VCC" pad="VIN"/>
<connect gate="G$1" pin="VOUT" pad="VOUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE" prefix="D">
<description>Oval pads for easier soldering.</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="1N400N" package="DO41">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1N4148" package="DO35">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="D-10">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RN09B" prefix="RN" uservalue="yes">
<description>&lt;b&gt;RESISTOR NETWORK: BUSSED:&lt;/b&gt; 9 resistor positions</description>
<gates>
<gate name="1" symbol="RN09"/>
</gates>
<devices>
<device name="" package="RN-10">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="10" pad="10"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="1" pin="3" pad="3"/>
<connect gate="1" pin="4" pad="4"/>
<connect gate="1" pin="5" pad="5"/>
<connect gate="1" pin="6" pad="6"/>
<connect gate="1" pin="7" pad="7"/>
<connect gate="1" pin="8" pad="8"/>
<connect gate="1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISP_HEADER" prefix="H">
<description>No more excuses for getting these lines crossed!</description>
<gates>
<gate name="G$1" symbol="ICSP"/>
</gates>
<devices>
<device name="" package="ICSP">
<connects>
<connect gate="G$1" pin="5V" pad="5"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="MISO" pad="6"/>
<connect gate="G$1" pin="MOSI" pad="3"/>
<connect gate="G$1" pin="RST" pad="2"/>
<connect gate="G$1" pin="SCK" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RN10B" prefix="RN" uservalue="yes">
<description>&lt;b&gt;RESISTOR NETWORK: BUSSED:&lt;/b&gt; 10 positions suitable for full bargraph</description>
<gates>
<gate name="1" symbol="RN10"/>
</gates>
<devices>
<device name="" package="RN-11">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="10" pad="10"/>
<connect gate="1" pin="11" pad="11"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="1" pin="3" pad="3"/>
<connect gate="1" pin="4" pad="4"/>
<connect gate="1" pin="5" pad="5"/>
<connect gate="1" pin="6" pad="6"/>
<connect gate="1" pin="7" pad="7"/>
<connect gate="1" pin="8" pad="8"/>
<connect gate="1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RN04I" prefix="RN" uservalue="yes">
<description>&lt;b&gt;RESISTOR NETWORK: ISOLATED&lt;/b&gt; (4 positions suitable for 7-Segment Displays&lt;br&gt;
More available in the &lt;b&gt;resistor-sil&lt;/b&gt; library</description>
<gates>
<gate name="A" symbol="RNV"/>
<gate name="B" symbol="RNV"/>
<gate name="C" symbol="RNV"/>
<gate name="D" symbol="RNV"/>
</gates>
<devices>
<device name="" package="SIL8">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="B" pin="1" pad="3"/>
<connect gate="B" pin="2" pad="4"/>
<connect gate="C" pin="1" pad="5"/>
<connect gate="C" pin="2" pad="6"/>
<connect gate="D" pin="1" pad="7"/>
<connect gate="D" pin="2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY85" prefix="MCU">
<description>&lt;b&gt;ATtiny85&lt;/b&gt; (Note: I've used the ATtiny13 symbol)</description>
<gates>
<gate name="G$1" symbol="ATTINY85"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0/PCINT0/AIN0/OC0A/MOSI" pad="5"/>
<connect gate="G$1" pin="PB1/PCINT1/AIN1/OC0B/INT0/MISO" pad="6"/>
<connect gate="G$1" pin="PB2/PCINT2/SCK/ADC1/T0" pad="7"/>
<connect gate="G$1" pin="PB3/PCINT3/CLKI/ADC3" pad="2"/>
<connect gate="G$1" pin="PB4/PCINT4/ADC2" pad="3"/>
<connect gate="G$1" pin="PB5/PCINT5/!RESET!/ADC0/DW" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRF540" prefix="Q">
<description>&lt;b&gt;N-Channel Enhancement MOSFET&lt;/b&gt; (HEXFET); 100V; 28A; 0,077Ohm</description>
<gates>
<gate name="G$1" symbol="IGFET-EN-GDS"/>
</gates>
<devices>
<device name="" package="TO220">
<connects>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TIP120" prefix="Q">
<description>&lt;b&gt;NPN DARLINGTON TRANSISTOR&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="N-DAR"/>
</gates>
<devices>
<device name="" package="TO220AH">
<connects>
<connect gate="1" pin="B" pad="B"/>
<connect gate="1" pin="C" pad="C"/>
<connect gate="1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ULN2803A" prefix="IC">
<description>&lt;b&gt;High Current Darlington Array:&lt;/b&gt; &lt;a href="http://www.ti.com/lit/ds/symlink/uln2803a.pdf"&gt;Datasheet&lt;/a&gt;
&lt;p&gt;Created on 2019 03 18 by C. D'Arcy.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ULN2803"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ULN2003A" prefix="IC">
<description>&lt;b&gt;High Current Darlington Array:&lt;/b&gt;
&lt;a href="http://www.ti.com/lit/ds/symlink/uln2003a.pdf"&gt;Datasheet&lt;/a&gt;
&lt;p&gt;Created on 2019 03 18 by C. D'Arcy.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ULN2003"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="COM" pad="9"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="2"/>
<connect gate="G$1" pin="IN3" pad="3"/>
<connect gate="G$1" pin="IN4" pad="4"/>
<connect gate="G$1" pin="IN5" pad="5"/>
<connect gate="G$1" pin="IN6" pad="6"/>
<connect gate="G$1" pin="IN7" pad="7"/>
<connect gate="G$1" pin="OUT1" pad="16"/>
<connect gate="G$1" pin="OUT2" pad="15"/>
<connect gate="G$1" pin="OUT3" pad="14"/>
<connect gate="G$1" pin="OUT4" pad="13"/>
<connect gate="G$1" pin="OUT5" pad="12"/>
<connect gate="G$1" pin="OUT6" pad="11"/>
<connect gate="G$1" pin="OUT7" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MSGEQ7" prefix="IC">
<description>A great tutorial (Neuwire: Skoba) can be found at:

&lt;a href="http://nuewire.com/info-archive/msgeq7-by-j-skoba/"&gt;http://nuewire.com/info-archive/msgeq7-by-j-skoba/&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="MSGEQ7"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="CLKIN" pad="8"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="IN" pad="5"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="RESET" pad="7"/>
<connect gate="G$1" pin="STROBE" pad="4"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS(GND)" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PORTHEADER6" prefix="H">
<description>Use for UNO Appliances to provide port access. Try to limit to 6 pins. (PORTB, PORTC, and PORTD).</description>
<gates>
<gate name="G$1" symbol="PINHD6"/>
</gates>
<devices>
<device name="" package="1X06/90">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="595" prefix="IC">
<description>If required, place a PWM signal on the G (/OE) pin 13 for fading (breathing) effects.</description>
<gates>
<gate name="G$1" symbol="74595"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="CLOCK" pad="11"/>
<connect gate="G$1" pin="DATA" pad="14"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="LATCH" pad="12"/>
<connect gate="G$1" pin="MR" pad="10"/>
<connect gate="G$1" pin="OE" pad="13"/>
<connect gate="G$1" pin="QA" pad="15"/>
<connect gate="G$1" pin="QB" pad="1"/>
<connect gate="G$1" pin="QC" pad="2"/>
<connect gate="G$1" pin="QD" pad="3"/>
<connect gate="G$1" pin="QE" pad="4"/>
<connect gate="G$1" pin="QF" pad="5"/>
<connect gate="G$1" pin="QG" pad="6"/>
<connect gate="G$1" pin="QH" pad="7"/>
<connect gate="G$1" pin="QH*" pad="9"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUDIO_JACK" prefix="J">
<description>&lt;b&gt;CONN JACK STEREO 3.5MM R/A&lt;/b&gt;
&lt;p&gt;&lt;b&gt;Digikey Part#:&lt;/b&gt; &lt;a href="https://www.digikey.ca/products/en?keywords=CP1-3524N-ND"&gt;CP1-3524N-ND&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Last Ordered (50): &lt;/b&gt; 2019 01 23&lt;p&gt;

&lt;p&gt;&lt;b&gt;NOTE:&lt;/b&gt; The SLEEVE of the 3.5 mm male jack is Ground. I've designed the&lt;b&gt;SLEEVE-to-GND&lt;/b&gt; board connection directly into this part to avoid the potential oversight. If for some reason this is not what you want find a similar part within the general EAGLE library collection.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="AUDIO_JACK"/>
</gates>
<devices>
<device name="" package="AUDIO_JACK">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="NP" pad="NP"/>
<connect gate="G$1" pin="RING" pad="RING"/>
<connect gate="G$1" pin="TIP" pad="TIP"/>
<connect gate="G$1" pin="TIP_SWITCH" pad="TIP_SWITCH"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SWITCHCRAFT" package="AUDIO_JACK_SWITCHCRAFT">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="NP" pad="R_SH"/>
<connect gate="G$1" pin="RING" pad="RING"/>
<connect gate="G$1" pin="TIP" pad="TIP"/>
<connect gate="G$1" pin="TIP_SWITCH" pad="T_SH"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="4_DIGIT_DISPLAY" prefix="L">
<description>&lt;b&gt;NOTE! Pin Layout valid for the following COMMON ANODE devices...&lt;/b&gt;
&lt;p&gt;
Digikey: &lt;a href="https://www.digikey.ca/products/en?keywords=160-1550-5-ND"&gt;RED: 160-1550-5-ND&lt;/a&gt;&lt;br&gt;
 &lt;a href="https://www.digikey.ca/products/en?keywords=160-1548-5-ND"&gt;YELLOW-ORANGE: 160-1548-5-ND&lt;/a&gt;&lt;br&gt;
&lt;a href="https://www.digikey.ca/product-detail/en/lite-on-inc/LTC-4627JS/160-1546-5-ND/408219"&gt;YELLOW: 160-1546-5-ND&lt;/a&gt;&lt;br&gt;
&lt;a href="https://www.digikey.ca/product-detail/en/vishay-semiconductor-opto-division/TDCG1060M/TDCG1060M-ND/4074707"&gt;GREEN: TDCG1060M-ND&lt;/a&gt;
&lt;p&gt; There are others available from other suppliers (ie ATA3492BW) but just make sure the CA pinouts agree.&lt;/p&gt;&lt;br&gt;
Use with &lt;b&gt;TPIC595 Power Shift Register&lt;/b&gt; for constant current sink.

&lt;p&gt;&lt;b&gt;Ordered: 2018 12 26&lt;/b&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="7-SEGMENT-4DIGIT-YOUNGSUN"/>
</gates>
<devices>
<device name="" package="7-SEGMENT-4DIGIT-YOUNGSUN-LONGPADS">
<connects>
<connect gate="G$1" pin="A" pad="14"/>
<connect gate="G$1" pin="APOS-A" pad="10"/>
<connect gate="G$1" pin="APOS-C" pad="9"/>
<connect gate="G$1" pin="B" pad="16"/>
<connect gate="G$1" pin="C" pad="13"/>
<connect gate="G$1" pin="COL-A" pad="4"/>
<connect gate="G$1" pin="COL-C" pad="12"/>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="DIG1" pad="1"/>
<connect gate="G$1" pin="DIG2" pad="2"/>
<connect gate="G$1" pin="DIG3" pad="6"/>
<connect gate="G$1" pin="DIG4" pad="8"/>
<connect gate="G$1" pin="DP" pad="7"/>
<connect gate="G$1" pin="E" pad="5"/>
<connect gate="G$1" pin="F" pad="11"/>
<connect gate="G$1" pin="G" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="8X8_MINI_MATRIX" prefix="L">
<description>&lt;b&gt;Acceptable pin Layout valid for the following ROW CATHODE devices include...&lt;/b&gt;
&lt;p&gt;
ABRA (your toolkit): &lt;a href="https://abra-electronics.com/opto-illumination/led-matrix/454-miniature-8x8-red-led-matrix-bl-m07c881ur-11-454-ada.html"&gt;RED: BL-M07C881UR-11&lt;/a&gt;&lt;br&gt;
Adafruit:&lt;br&gt;
&lt;a href="https://www.adafruit.com/product/956"&gt;BLUE: KWM-20882CBA&lt;/a&gt;&lt;br&gt;
&lt;a href="https://www.adafruit.com/product/454"&gt;HYPER RED: KWM-20882CVB&lt;/a&gt;&lt;br&gt;
&lt;a href="https://www.adafruit.com/product/1079"&gt;ULTRA WHITE: KWM-20882CWB-Y&lt;/a&gt;&lt;br&gt;
&lt;a href="https://www.adafruit.com/product/861"&gt;YELLOW GREEN: KWM-20882CUGB&lt;/a&gt;&lt;br&gt; 
&lt;a href="https://www.adafruit.com/product/860"&gt;YELLOW: KWM-20882CUYB&lt;/a&gt;&lt;br&gt; 


&lt;p&gt;There are others available from other suppliers  but just make sure they're ID'd as &lt;b&gt;ROW CATHODE&lt;/b&gt; and the pinouts agree.&lt;/p&gt;
&lt;p&gt;Created on 2019 03 18 by C. D'Arcy.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SEGMENT_8X8_CATHODEROW"/>
</gates>
<devices>
<device name="" package="SEGMENT_BL-M07C881UR">
<connects>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A2" pad="6"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="8"/>
<connect gate="G$1" pin="A5" pad="16"/>
<connect gate="G$1" pin="A6" pad="15"/>
<connect gate="G$1" pin="A7" pad="14"/>
<connect gate="G$1" pin="A8" pad="13"/>
<connect gate="G$1" pin="K1" pad="1"/>
<connect gate="G$1" pin="K2" pad="2"/>
<connect gate="G$1" pin="K3" pad="3"/>
<connect gate="G$1" pin="K4" pad="4"/>
<connect gate="G$1" pin="K5" pad="12"/>
<connect gate="G$1" pin="K6" pad="11"/>
<connect gate="G$1" pin="K7" pad="10"/>
<connect gate="G$1" pin="K8" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MINI_USB" prefix="J">
<description>MINI USB-B R/A DIP&lt;/b&gt; 5pol.&lt;p&gt;
Source: www.cypressindustries.com</description>
<gates>
<gate name="G41" symbol="MINI-USB-5"/>
<gate name="S" symbol="SHIELD2"/>
</gates>
<devices>
<device name="32005-601" package="MINI_USB">
<connects>
<connect gate="G41" pin="2" pad="2"/>
<connect gate="G41" pin="3" pad="3"/>
<connect gate="G41" pin="4" pad="4"/>
<connect gate="G41" pin="GND" pad="5"/>
<connect gate="G41" pin="VIN" pad="1"/>
<connect gate="S" pin="S1" pad="M1"/>
<connect gate="S" pin="S2" pad="M2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CR1220" prefix="B">
<description>&lt;b&gt;CR1220&lt;/b&gt; PTH Battery Holder for &lt;b&gt;DS1307 RTCs&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="BATTERY"/>
</gates>
<devices>
<device name="" package="BATTCON_12MM_PTH">
<connects>
<connect gate="G$1" pin="+" pad="VCC@1 VCC@2"/>
<connect gate="G$1" pin="-" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPIC6C595" prefix="IC">
<description>&lt;b&gt;Power-Logic 8-Bit Shift Register:&lt;/b&gt; &lt;a href="http://www.ti.com/lit/ds/symlink/tpic6c595.pdf"&gt;Datasheet&lt;/a&gt;
&lt;p&gt;Added: 2019 03 18 by C. D'Arcy.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TPIC6C595"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="/CLR" pad="7"/>
<connect gate="G$1" pin="DRAIN0" pad="3"/>
<connect gate="G$1" pin="DRAIN1" pad="4"/>
<connect gate="G$1" pin="DRAIN2" pad="5"/>
<connect gate="G$1" pin="DRAIN3" pad="6"/>
<connect gate="G$1" pin="DRAIN4" pad="11"/>
<connect gate="G$1" pin="DRAIN5" pad="12"/>
<connect gate="G$1" pin="DRAIN6" pad="13"/>
<connect gate="G$1" pin="DRAIN7" pad="14"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="RCK" pad="10"/>
<connect gate="G$1" pin="SCK" pad="15"/>
<connect gate="G$1" pin="SCL" pad="8"/>
<connect gate="G$1" pin="SER_IN" pad="2"/>
<connect gate="G$1" pin="SER_OUT" pad="9"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED_RGB_CA">
<gates>
<gate name="G$1" symbol="LED-RGB-CA"/>
</gates>
<devices>
<device name="" package="LED_RGB_CA">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="BLU" pad="4"/>
<connect gate="G$1" pin="GRN" pad="3"/>
<connect gate="G$1" pin="RED" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED_RGB_CC" prefix="LED">
<gates>
<gate name="G$1" symbol="LED-RGB-CC"/>
</gates>
<devices>
<device name="" package="LED_RGB_CC">
<connects>
<connect gate="G$1" pin="BLU" pad="4"/>
<connect gate="G$1" pin="C" pad="GND"/>
<connect gate="G$1" pin="GRN" pad="3"/>
<connect gate="G$1" pin="RED" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESONATOR" prefix="X">
<description>Inexpensive but less reliable alternative to 16MHz crystal and 22&amp;rho;F filter caps for offboard ATmega328p.</description>
<gates>
<gate name="G$1" symbol="RESONATOR"/>
</gates>
<devices>
<device name="" package="RESONATOR-PTH-7.6X3.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUDIO_AMP" prefix="IC">
<description>&lt;b&gt;1 W BTL mono audio amplifier with DC volume control&lt;/b&gt;
&lt;p&gt;&lt;a href="https://www.nxp.com/docs/en/data-sheet/TDA7052A_AT.pdf?"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;

&lt;p&gt;Here's a &lt;a href="http://rheslip.blogspot.com/2012/04/tda7052a-audio-amp-with-agc-and-mute_23.html"&gt;blog&lt;/a&gt; that describes IC's use in a headphoe application.&lt;/p&gt;


Used in E. MacAuliffe's &lt;a href="https://blog.emcauliffe.ca/2018/03/10/Photophone.html"&gt;Photophone&lt;/a&gt;

&lt;p&gt;&lt;b&gt;Last Ordered&lt;/b&gt;: ABRA (No longer in production)&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Digikey Part #&lt;/b&gt;: &lt;a href="https://www.digikey.ca/product-detail/en/nxp-usa-inc/TDA7052A-N2112/568-1138-5-ND/735752"&gt;568-1138-5-ND&lt;/a&gt; (Obsolete)&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TDA7052A"/>
</gates>
<devices>
<device name="" package="TDA7052A">
<connects>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="IN+" pad="INPUT"/>
<connect gate="G$1" pin="NC" pad="NC7"/>
<connect gate="G$1" pin="NC4" pad="NC4"/>
<connect gate="G$1" pin="OUT+" pad="OUT5"/>
<connect gate="G$1" pin="OUT-" pad="OUT8"/>
<connect gate="G$1" pin="VP" pad="VP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HD44780LCD" prefix="LCD">
<description>Adafruit Part #1447: &lt;b&gt;&lt;a href="https://www.adafruit.com/product/1447"&gt;HD44780 LCD&lt;/a&gt;&lt;/b&gt;
&lt;p&gt;&lt;a href="https://cdn-shop.adafruit.com/datasheets/TC1602A-01T.pdf"&gt;&lt;b&gt;Datasheet&lt;/b&gt;&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Standard character type LCDs, available in sizes from 8x1 to 40x4!&lt;/p&gt;
&lt;p&gt;Standard Arduino Library: Adafruit's &lt;a href="https://github.com/adafruit/Adafruit_LiquidCrystal"&gt;&lt;b&gt;LiquidCrystal&lt;/b&gt;&lt;/a&gt; Library on GitHub.&lt;/p&gt;
&lt;p&gt;Adafruit's &lt;a href="https://learn.adafruit.com/character-lcdsl"&gt;&lt;b&gt;Tutorial&lt;/b&gt;&lt;/a&gt;.&lt;/p&gt;
&lt;hr width="50%" &gt;
Use with: &lt;a href="http://darcy.rsgc.on.ca/ACES/PCBs/index.html#LCD"&gt;RSGC ACES 16&amp;times;2 Character LCD Carrier Appliance&lt;/a&gt;.
&lt;p&gt;HD44780U Control Driver IC: &lt;A href="https://cdn-shop.adafruit.com/datasheets/HD44780.pdf"&gt;&lt;b&gt;Datasheet&lt;/b&gt;&lt;/a&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CLCD"/>
</gates>
<devices>
<device name="-1602" package="LCD1602">
<connects>
<connect gate="G$1" pin="A" pad="15"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="K" pad="16"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="RW" pad="5"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VO" pad="3"/>
<connect gate="G$1" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7_SEGMENT" prefix="L">
<description>&lt;b&gt;LED DISPLAY&lt;/b&gt;&lt;p&gt;
 1-character 7 segment, decimal point right
&lt;p&gt;Taken from&lt;b&gt;display-hp&lt;/b&gt; library: HD-H101&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="HD7"/>
</gates>
<devices>
<device name="COMMON_CATHODE" package="HDSP">
<connects>
<connect gate="G$1" pin="A" pad="7"/>
<connect gate="G$1" pin="B" pad="6"/>
<connect gate="G$1" pin="C" pad="4"/>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="DP" pad="5"/>
<connect gate="G$1" pin="E" pad="1"/>
<connect gate="G$1" pin="F" pad="9"/>
<connect gate="G$1" pin="G" pad="10"/>
<connect gate="G$1" pin="S3" pad="3"/>
<connect gate="G$1" pin="S8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="COMMON_ANODE" package="HDSP">
<connects>
<connect gate="G$1" pin="A" pad="7"/>
<connect gate="G$1" pin="B" pad="6"/>
<connect gate="G$1" pin="C" pad="4"/>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="DP" pad="5"/>
<connect gate="G$1" pin="E" pad="1"/>
<connect gate="G$1" pin="F" pad="9"/>
<connect gate="G$1" pin="G" pad="10"/>
<connect gate="G$1" pin="S3" pad="3"/>
<connect gate="G$1" pin="S8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOUNTING_HOLE">
<description>&lt;p&gt;For consistency, ACES use 3mm &lt;a href="https://www.mcmaster.com/92492a715"&gt;screws&lt;/a&gt; and &lt;a href="https://www.mcmaster.com/94180a333"&gt;heat set inserts&lt;/a&gt; from McMaster-Carr for their PCB and Case designs.&lt;/p&gt;

&lt;p&gt;These holes were ported from the microbuilder library and offer no ground protection as we typically use nylon hardware.&lt;/p&gt;
&lt;p&gt;You are encouraged to use this these mounting  holes for your PCB designs.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MOUNTING_HOLE"/>
</gates>
<devices>
<device name="" package="MOUNTINGHOLE_3.2MM_PLATEDTHIN">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC0804" prefix="IC">
<gates>
<gate name="G$1" symbol="ADC0804"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="/CS" pad="1"/>
<connect gate="G$1" pin="/INTR" pad="5"/>
<connect gate="G$1" pin="/RD" pad="2"/>
<connect gate="G$1" pin="/WR" pad="3"/>
<connect gate="G$1" pin="AGND" pad="8"/>
<connect gate="G$1" pin="CLK_IN" pad="4"/>
<connect gate="G$1" pin="CLK_R" pad="19"/>
<connect gate="G$1" pin="DB0" pad="18"/>
<connect gate="G$1" pin="DB1" pad="17"/>
<connect gate="G$1" pin="DB2" pad="16"/>
<connect gate="G$1" pin="DB3" pad="15"/>
<connect gate="G$1" pin="DB4" pad="14"/>
<connect gate="G$1" pin="DB5" pad="13"/>
<connect gate="G$1" pin="DB6" pad="12"/>
<connect gate="G$1" pin="DB7" pad="11"/>
<connect gate="G$1" pin="DGND" pad="10"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="VIN+" pad="6"/>
<connect gate="G$1" pin="VIN-" pad="7"/>
<connect gate="G$1" pin="VREF/2" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RN08B" prefix="L">
<description>&lt;p&gt;&lt;b&gt;RESISTOR NETWORK: BUSSED:&lt;/b&gt; 8 positions suitable for binary byte display on a bargraph</description>
<gates>
<gate name="L$1" symbol="RN08"/>
</gates>
<devices>
<device name="" package="RN-9">
<connects>
<connect gate="L$1" pin="1" pad="1"/>
<connect gate="L$1" pin="2" pad="2"/>
<connect gate="L$1" pin="3" pad="3"/>
<connect gate="L$1" pin="4" pad="4"/>
<connect gate="L$1" pin="5" pad="5"/>
<connect gate="L$1" pin="6" pad="6"/>
<connect gate="L$1" pin="7" pad="7"/>
<connect gate="L$1" pin="8" pad="8"/>
<connect gate="L$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT28C16" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2816"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL24">
<connects>
<connect gate="A" pin="!CE" pad="18"/>
<connect gate="A" pin="!OE" pad="20"/>
<connect gate="A" pin="!WE" pad="21"/>
<connect gate="A" pin="A0" pad="8"/>
<connect gate="A" pin="A1" pad="7"/>
<connect gate="A" pin="A10" pad="19"/>
<connect gate="A" pin="A2" pad="6"/>
<connect gate="A" pin="A3" pad="5"/>
<connect gate="A" pin="A4" pad="4"/>
<connect gate="A" pin="A5" pad="3"/>
<connect gate="A" pin="A6" pad="2"/>
<connect gate="A" pin="A7" pad="1"/>
<connect gate="A" pin="A8" pad="23"/>
<connect gate="A" pin="A9" pad="22"/>
<connect gate="A" pin="D0" pad="9"/>
<connect gate="A" pin="D1" pad="10"/>
<connect gate="A" pin="D2" pad="11"/>
<connect gate="A" pin="D3" pad="13"/>
<connect gate="A" pin="D4" pad="14"/>
<connect gate="A" pin="D5" pad="15"/>
<connect gate="A" pin="D6" pad="16"/>
<connect gate="A" pin="D7" pad="17"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="+5V" prefix="P+">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="+5V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VCC" prefix="P+">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="VCC" symbol="VCC"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="14_SEGMENT_DUAL_CC" prefix="LED">
<description>&lt;p&gt;Lite-On's &lt;b&gt;LTP-3784&lt;/b&gt; Green Dual 14-Segment &lt;b&gt;CC&lt;/b&gt; Display.&lt;/p&gt;
Digikey Part# &lt;b&gt;160-1012-ND&lt;/b&gt; (also comes in RED-ORNG: 160-1010-N)&lt;br&gt;
Used in 19/20 ICS3U &lt;a href="http://darcy.rsgc.on.ca/ACES/TEI3M/1920/Tasks.html#PoV" target="_blank"&gt;PoV Word&lt;/a&gt; Project&lt;br&gt;
Designed 2020 01 05 for J. Buchan's Legacy PCB Project.</description>
<gates>
<gate name="G$1" symbol="14-SEG-LED-DUAL-C"/>
</gates>
<devices>
<device name="" package="DUAL_CC_14-SEGMENT">
<connects>
<connect gate="G$1" pin="A" pad="12"/>
<connect gate="G$1" pin="B" pad="10"/>
<connect gate="G$1" pin="C" pad="9"/>
<connect gate="G$1" pin="CC1" pad="16"/>
<connect gate="G$1" pin="CC2" pad="11"/>
<connect gate="G$1" pin="D" pad="7"/>
<connect gate="G$1" pin="DP" pad="8"/>
<connect gate="G$1" pin="E" pad="1"/>
<connect gate="G$1" pin="F" pad="18"/>
<connect gate="G$1" pin="G" pad="15"/>
<connect gate="G$1" pin="H" pad="14"/>
<connect gate="G$1" pin="J" pad="6"/>
<connect gate="G$1" pin="K" pad="5"/>
<connect gate="G$1" pin="L" pad="4"/>
<connect gate="G$1" pin="M" pad="2"/>
<connect gate="G$1" pin="N" pad="13"/>
<connect gate="G$1" pin="P" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EG1218" prefix="S" uservalue="yes">
<description>&lt;b&gt;SLIDING SWITCH&lt;/b&gt;&lt;p&gt;
0.1" spacing through hole, vertical SPDT slide switch
&lt;p&gt;http://www.ladyada.net/library/pcb/eaglelibrary.html&lt;/p&gt;</description>
<gates>
<gate name="1" symbol="SIS"/>
</gates>
<devices>
<device name="S" package="EG1218">
<connects>
<connect gate="1" pin="O" pad="O"/>
<connect gate="1" pin="P" pad="P"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUDIO_JACK_SWITCHCRAFT">
<gates>
<gate name="G$1" symbol="AUDIO_JACK_SWITCHCRAFT"/>
</gates>
<devices>
<device name="" package="AUDIO_JACK_SWITCHCRAFT">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="RING" pad="RING"/>
<connect gate="G$1" pin="TIP" pad="TIP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
