<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="40.63" x2="0" y2="2.54" width="0" layer="20"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0" layer="20" curve="90"/>
<wire x1="2.54" y1="0" x2="63.17" y2="0" width="0" layer="20"/>
<wire x1="63.17" y1="0" x2="65.71" y2="2.54" width="0" layer="20" curve="90"/>
<wire x1="65.71" y1="2.54" x2="65.71" y2="40.63" width="0" layer="20"/>
<wire x1="65.71" y1="40.63" x2="63.17" y2="43.17" width="0" layer="20" curve="90"/>
<wire x1="63.17" y1="43.17" x2="2.54" y2="43.17" width="0" layer="20"/>
<wire x1="2.54" y1="43.17" x2="0" y2="40.63" width="0" layer="20" curve="90"/>
<text>Morland Shift-Bargraph Appliance. SMT Version.</text>
<text>GR DA CL LA</text>
<text>EN INT0</text>
<text>INT0</text>
<text>5VDC</text>
<text>5VDC</text>
<text>INT0</text>
<text>C:/Users/Chris Darcy/Desktop/EAGLE Tips/ACESLogov2.bmp</text>
<text>RSGC ACES</text>
<text>Your Name. 2019.</text>
</plain>
<libraries>
<library name="SparkFun-IC-Logic">
<description>&lt;h3&gt;SparkFun Logic ICs&lt;/h3&gt;
This library contains parts which fit into the standard logic IC families.&lt;br&gt;&lt;br&gt;
This library is special as the devices are most generalized, with manufacturer specific variants stemming from the generalized numbers.  It also uses individual gates for common parts with a power consort.  Place the gates in a schematic such that they are easy to see in the circuit, and apply power to the power symbol for multigate packages. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO16">
<description>SOIC, 0.15 inch width</description>
</package>
</packages>
</library>
<library name="resistor-bourns">
<description>&lt;b&gt;Bourns Resistor Networks&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="4816P">
<description>&lt;b&gt;BOURNS RESISTOR NETWORK&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
<description>&lt;h3&gt;LED 1206 SMT&lt;/h3&gt;

1206, surface mount. 

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: &lt;/li&gt;
&lt;li&gt;Area: 0.125" x 0.06"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="1X2-3.5MM">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-hirose">
<description>&lt;b&gt;Hirose Connectors&lt;/b&gt;&lt;p&gt;
www.hirose.co.jp&lt;p&gt;
Include : &lt;br&gt;
con-hirose-df12d(3.0)60dp0.5v80.lbr from Bob Starr &amp;lt;rtzaudio@mindspring.com&amp;gt;&lt;br&gt;
con-hirose.lbr from Bob Starr &amp;lt;rtzaudio@mindspring.com&amp;gt;&lt;br&gt;</description>
<packages>
<package name="UX60-MB-5ST">
<description>&lt;b&gt;MINI USB Connector HI-SPEED Certified&lt;/b&gt; Metal Shield SMT Type With Positioning Post&lt;p&gt;
Source: http://www.hirose.co.jp/cataloge_hp/e24000019.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-AB-MICRO-SMD">
<description>&lt;h3&gt;USB Type AB - SMT&lt;/h3&gt;
&lt;br&gt; Basic silk outline&lt;/br&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5 main, 3 shield&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint: http://www.morethanall.com//upload/products_pdf/87340574052ba5151280ca.pdf&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB AB&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="SparkFun-IC-Logic" package="SO16" value="SN74HC595D">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-07875"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="SparkFun-IC-Logic" package="SO16" value="SN74HC595D">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-07875"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="SparkFun-IC-Logic" package="SO16" value="SN74HC595D">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-07875"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="resistor-bourns" package="4816P" value="">
<attribute name="MF" value="BOURNS, INC."/>
<attribute name="MPN" value="4816P-T01-684LF"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="9357483"/>
<attribute name="OC_NEWARK" value="33K0707"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="resistor-bourns" package="4816P" value="">
<attribute name="MF" value="BOURNS, INC."/>
<attribute name="MPN" value="4816P-T01-684LF"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="9357483"/>
<attribute name="OC_NEWARK" value="33K0707"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="resistor-bourns" package="4816P" value="">
<attribute name="MF" value="BOURNS, INC."/>
<attribute name="MPN" value="4816P-T01-684LF"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="9357483"/>
<attribute name="OC_NEWARK" value="33K0707"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D7" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D8" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D9" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D10" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D11" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D12" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D13" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D14" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D15" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D16" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D17" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D18" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D19" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D20" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D21" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D22" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D23" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D24" library="SparkFun-LED" package="LED-1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="adafruit" package="1X2-3.5MM" value="1X2-3.5MM">
<attribute name="NAME"/>
</element>
<element name="JP1" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="pinhead" package="1X02/90" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="pinhead" package="1X04/90" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="con-hirose" package="UX60-MB-5ST" value="MINI-USB-SHIELD-UX60-MB-5ST">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="USB-AB-MICRO-SMD" value="">
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-11794"/>
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="JP4" pad="4"/>
<contactref element="U3" pad="8"/>
<contactref element="U2" pad="8"/>
<contactref element="U1" pad="8"/>
<contactref element="D24" pad="C"/>
<contactref element="D23" pad="C"/>
<contactref element="D22" pad="C"/>
<contactref element="D21" pad="C"/>
<contactref element="D20" pad="C"/>
<contactref element="D19" pad="C"/>
<contactref element="D18" pad="C"/>
<contactref element="D17" pad="C"/>
<contactref element="D16" pad="C"/>
<contactref element="D15" pad="C"/>
<contactref element="D14" pad="C"/>
<contactref element="D13" pad="C"/>
<contactref element="D12" pad="C"/>
<contactref element="D11" pad="C"/>
<contactref element="D10" pad="C"/>
<contactref element="D9" pad="C"/>
<contactref element="D8" pad="C"/>
<contactref element="D7" pad="C"/>
<contactref element="D6" pad="C"/>
<contactref element="D5" pad="C"/>
<contactref element="D4" pad="C"/>
<contactref element="D3" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="D1" pad="C"/>
<contactref element="J2" pad="GND1"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="16"/>
<contactref element="J1" pad="2"/>
<contactref element="U2" pad="16"/>
<contactref element="U3" pad="16"/>
<contactref element="JP1" pad="1"/>
<contactref element="U1" pad="10"/>
<contactref element="U2" pad="10"/>
<contactref element="U3" pad="10"/>
</signal>
<signal name="N$1">
<contactref element="D1" pad="A"/>
<contactref element="R1" pad="9"/>
</signal>
<signal name="N$2">
<contactref element="D2" pad="A"/>
<contactref element="R1" pad="10"/>
</signal>
<signal name="N$3">
<contactref element="D3" pad="A"/>
<contactref element="R1" pad="11"/>
</signal>
<signal name="N$4">
<contactref element="D4" pad="A"/>
<contactref element="R1" pad="12"/>
</signal>
<signal name="N$5">
<contactref element="D5" pad="A"/>
<contactref element="R1" pad="13"/>
</signal>
<signal name="N$6">
<contactref element="D6" pad="A"/>
<contactref element="R1" pad="14"/>
</signal>
<signal name="N$7">
<contactref element="D7" pad="A"/>
<contactref element="R1" pad="15"/>
</signal>
<signal name="N$8">
<contactref element="D8" pad="A"/>
<contactref element="R1" pad="16"/>
</signal>
<signal name="N$9">
<contactref element="D9" pad="A"/>
<contactref element="R2" pad="9"/>
</signal>
<signal name="N$10">
<contactref element="D10" pad="A"/>
<contactref element="R2" pad="10"/>
</signal>
<signal name="N$11">
<contactref element="D11" pad="A"/>
<contactref element="R2" pad="11"/>
</signal>
<signal name="N$12">
<contactref element="D12" pad="A"/>
<contactref element="R2" pad="12"/>
</signal>
<signal name="N$13">
<contactref element="D13" pad="A"/>
<contactref element="R2" pad="13"/>
</signal>
<signal name="N$14">
<contactref element="D14" pad="A"/>
<contactref element="R2" pad="14"/>
</signal>
<signal name="N$15">
<contactref element="D15" pad="A"/>
<contactref element="R2" pad="15"/>
</signal>
<signal name="N$16">
<contactref element="D16" pad="A"/>
<contactref element="R2" pad="16"/>
</signal>
<signal name="N$17">
<contactref element="D17" pad="A"/>
<contactref element="R3" pad="9"/>
</signal>
<signal name="N$18">
<contactref element="D18" pad="A"/>
<contactref element="R3" pad="10"/>
</signal>
<signal name="N$19">
<contactref element="D19" pad="A"/>
<contactref element="R3" pad="11"/>
</signal>
<signal name="N$20">
<contactref element="D20" pad="A"/>
<contactref element="R3" pad="12"/>
</signal>
<signal name="N$21">
<contactref element="D21" pad="A"/>
<contactref element="R3" pad="13"/>
</signal>
<signal name="N$22">
<contactref element="D22" pad="A"/>
<contactref element="R3" pad="14"/>
</signal>
<signal name="N$23">
<contactref element="D23" pad="A"/>
<contactref element="R3" pad="15"/>
</signal>
<signal name="N$24">
<contactref element="D24" pad="A"/>
<contactref element="R3" pad="16"/>
</signal>
<signal name="LATCH">
<contactref element="JP4" pad="1"/>
<contactref element="U2" pad="12"/>
<contactref element="U1" pad="12"/>
<contactref element="U3" pad="12"/>
</signal>
<signal name="DATA">
<contactref element="JP4" pad="3"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="EN">
<contactref element="JP3" pad="2"/>
<contactref element="U3" pad="13"/>
<contactref element="U2" pad="13"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="INT0">
<contactref element="JP3" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="CLOCK">
<contactref element="JP4" pad="2"/>
<contactref element="U2" pad="11"/>
<contactref element="U1" pad="11"/>
<contactref element="U3" pad="11"/>
</signal>
<signal name="DATAOUT1">
<contactref element="U1" pad="9"/>
<contactref element="U2" pad="14"/>
</signal>
<signal name="DATAOUT2">
<contactref element="U2" pad="9"/>
<contactref element="U3" pad="14"/>
</signal>
<signal name="R1_1">
<contactref element="U1" pad="15"/>
<contactref element="R1" pad="8"/>
</signal>
<signal name="R1_3">
<contactref element="U1" pad="2"/>
<contactref element="R1" pad="6"/>
</signal>
<signal name="R1_4">
<contactref element="U1" pad="3"/>
<contactref element="R1" pad="5"/>
</signal>
<signal name="R1_5">
<contactref element="U1" pad="4"/>
<contactref element="R1" pad="4"/>
</signal>
<signal name="R1_6">
<contactref element="U1" pad="5"/>
<contactref element="R1" pad="3"/>
</signal>
<signal name="R1_7">
<contactref element="U1" pad="6"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="R1_8">
<contactref element="U1" pad="7"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="R1_2">
<contactref element="R1" pad="7"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="R2_1">
<contactref element="U2" pad="15"/>
<contactref element="R2" pad="8"/>
</signal>
<signal name="R2_2">
<contactref element="U2" pad="1"/>
<contactref element="R2" pad="7"/>
</signal>
<signal name="R2_3">
<contactref element="U2" pad="2"/>
<contactref element="R2" pad="6"/>
</signal>
<signal name="R2_4">
<contactref element="U2" pad="3"/>
<contactref element="R2" pad="5"/>
</signal>
<signal name="R2_5">
<contactref element="U2" pad="4"/>
<contactref element="R2" pad="4"/>
</signal>
<signal name="R2_6">
<contactref element="U2" pad="5"/>
<contactref element="R2" pad="3"/>
</signal>
<signal name="R2_7">
<contactref element="U2" pad="6"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="R2_8">
<contactref element="U2" pad="7"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="R3_1">
<contactref element="U3" pad="15"/>
<contactref element="R3" pad="8"/>
</signal>
<signal name="R3_2">
<contactref element="U3" pad="1"/>
<contactref element="R3" pad="7"/>
</signal>
<signal name="R3_3">
<contactref element="U3" pad="2"/>
<contactref element="R3" pad="6"/>
</signal>
<signal name="R3_4">
<contactref element="U3" pad="3"/>
<contactref element="R3" pad="5"/>
</signal>
<signal name="R3_5">
<contactref element="U3" pad="4"/>
<contactref element="R3" pad="4"/>
</signal>
<signal name="R3_6">
<contactref element="U3" pad="5"/>
<contactref element="R3" pad="3"/>
</signal>
<signal name="R3_7">
<contactref element="U3" pad="6"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="R3_8">
<contactref element="U3" pad="7"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="VBUS">
<contactref element="J2" pad="VBUS1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
