<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="48" x2="0" y2="2" width="0" layer="20"/>
<wire x1="0" y1="2" x2="2" y2="0" width="0" layer="20" curve="90"/>
<wire x1="2" y1="0" x2="30" y2="0" width="0" layer="20"/>
<wire x1="30" y1="0" x2="32" y2="2" width="0" layer="20" curve="90"/>
<wire x1="32" y1="2" x2="32" y2="48" width="0" layer="20"/>
<wire x1="32" y1="48" x2="30" y2="50" width="0" layer="20" curve="90"/>
<wire x1="30" y1="50" x2="2" y2="50" width="0" layer="20"/>
<wire x1="2" y1="50" x2="0" y2="48" width="0" layer="20" curve="90"/>
<text>MatrixMadeEZv2</text>
<text>HUGO REED</text>
<text>RSGC ACES. 2018</text>
<text>DESIGN ENGINEERING STUDIO</text>
<text> 8   7   6   5   4   3   2   1</text>
<text>1   2   3   4   5   6   7   8</text>
<text>5V DA CK</text>
<text>LA DM GD</text>
<text>TPIC6C595</text>
<text>SN74HC595</text>
<text>^MATRIX SILK SCREENING^</text>
<text>COMPATIBLE MATRICES
KWM-20882CWB-Y
BL-M07C881UR</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin with Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="SEGMENT_BL-M07C881UR">
</package>
</packages>
</library>
<library name="ic-package">
<description>&lt;b&gt;IC Packages an Sockets&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J2" library="SparkFun-Connectors" package="1X06_LONGPADS" value=""/>
<element name="LEDMATRIX" library="adafruit" package="SEGMENT_BL-M07C881UR" value="BL-M07C881UR-11"/>
<element name="IC1" library="ic-package" package="DIL16" value="TPIC6C595"/>
<element name="IC2" library="ic-package" package="DIL16" value="SN74HC595"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="J2" pad="1"/>
<contactref element="IC2" pad="16"/>
<contactref element="IC2" pad="10"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="DATA">
<contactref element="J2" pad="2"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="CLOCK">
<contactref element="J2" pad="3"/>
<contactref element="IC2" pad="11"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="LATCH">
<contactref element="J2" pad="4"/>
<contactref element="IC2" pad="12"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="GND">
<contactref element="IC2" pad="8"/>
<contactref element="IC2" pad="13"/>
<contactref element="IC1" pad="16"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="ROW1">
<contactref element="IC1" pad="3"/>
<contactref element="LEDMATRIX" pad="1"/>
</signal>
<signal name="ROW2">
<contactref element="IC1" pad="4"/>
<contactref element="LEDMATRIX" pad="2"/>
</signal>
<signal name="ROW3">
<contactref element="IC1" pad="5"/>
<contactref element="LEDMATRIX" pad="3"/>
</signal>
<signal name="ROW4">
<contactref element="IC1" pad="6"/>
<contactref element="LEDMATRIX" pad="4"/>
</signal>
<signal name="ROW5">
<contactref element="IC1" pad="11"/>
<contactref element="LEDMATRIX" pad="12"/>
</signal>
<signal name="ROW6">
<contactref element="IC1" pad="12"/>
<contactref element="LEDMATRIX" pad="11"/>
</signal>
<signal name="ROW7">
<contactref element="IC1" pad="13"/>
<contactref element="LEDMATRIX" pad="10"/>
</signal>
<signal name="ROW8">
<contactref element="IC1" pad="14"/>
<contactref element="LEDMATRIX" pad="9"/>
</signal>
<signal name="COL2">
<contactref element="IC2" pad="1"/>
<contactref element="LEDMATRIX" pad="6"/>
</signal>
<signal name="COL3">
<contactref element="IC2" pad="2"/>
<contactref element="LEDMATRIX" pad="7"/>
</signal>
<signal name="COL4">
<contactref element="IC2" pad="3"/>
<contactref element="LEDMATRIX" pad="8"/>
</signal>
<signal name="COL5">
<contactref element="IC2" pad="4"/>
<contactref element="LEDMATRIX" pad="16"/>
</signal>
<signal name="COL6">
<contactref element="IC2" pad="5"/>
<contactref element="LEDMATRIX" pad="15"/>
</signal>
<signal name="COL7">
<contactref element="IC2" pad="6"/>
<contactref element="LEDMATRIX" pad="14"/>
</signal>
<signal name="COL8">
<contactref element="IC2" pad="7"/>
<contactref element="LEDMATRIX" pad="13"/>
</signal>
<signal name="QH'">
<contactref element="IC2" pad="9"/>
</signal>
<signal name="COL1">
<contactref element="IC2" pad="15"/>
<contactref element="LEDMATRIX" pad="5"/>
</signal>
<signal name="DATAOUT">
<contactref element="IC2" pad="14"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="DIM">
<contactref element="J2" pad="5"/>
<contactref element="IC1" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
