Open the Falstad Circuit Simulation applet (<https://www.falstad.com/circuit/>).

Under the **File** menu, select **New Blank Circuit**.

Recreate the **Switched LED** circuit shown below. Run to confirm.

**Note.** If you find this applet useful for you DER schematics, be sure to first invert the background colour (**Options>White Background**) before undertaking your screen capture as I have done here.

